{"text_format":"1","workbook":"xlsx","n_sheets":13,"sheets":["READ ME","SBTM","iSBTM","STAB","STAB OUTPUT","STAB plot DATA","STATE","STATE I OUTPUT","STATE II OUTPUT","STATE plot DATA","qt chart","SBTMzt","SBTMsa"],"not_rendered":{"charts":16,"images":15,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"READ ME","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"SBTM","index":1,"n_rows":41,"n_cols":16,"rows_kept":41,"cut":false,"hidden":false,"merged":[[18,9,18,12],[19,9,19,11]]}
["SBTM - calculate transport rate and transport grain size from"]
[null,"specified shear velocity and bed surface grain size"]
["RULES, CONVENTIONS, AND UNITS"]
["1. Cells for input data are highlighted in GREEN, cells for output data are ORANGE"]
["2. Grain-diameters must be in millimeters (mm)"]
["3. Cumulative percentiles, not fractions, are used"]
["4. Cumulative grain-size distribution percentiles must span from 0 to 100 %"]
["5. Shear velocity must be in meters-per-second (m/s)"]
["6. The 0 and 100 % must be EXACTLY 0 and 100"]
["INSTRUCTIONS"]
["1. In table below, enter grain size and cumulative % in order of decreasing grain size"]
["2. Enter your bed shear velocity"]
["3. Check input for errors, press Enter, and then click once on the Run SBTM button"]
[]
["Parameter","Value","Description","Units"]
["u*",0.2,"Bed shear velocity","m/s",null,null,null,null,null,"This worksheet calculates transport rates per unit width in units of m2/s"]
["qT",3.2394888182298183E-4,"Total transport rate","m2/s",null,null,null,null,null,"    (m3 of solid sediment per m of channel width per s = m2/s)"]
[null,null,null,null,null,null,null,null,null,"as a function of shear velocity in units of m/s. Here are some convenient unit conversions."]
["D (mm)","Surface CDF GSD (% Finer)","Transport CDF GSD (% Finer)",null,"Statistic","Surface GSD","Transport GSD","Units",null,"Handy Conversion Table",null,null,null,"Input"]
[64,100,100,null,"Dmin",2.83,2.83,"mm",null,"From",null,null,"To","Output"]
[45.25,93.670886075949369,98.321066504914327,null,"Dmax",64,64,"mm",null,null,null,"Shear Stress","Shear Velocity",1000,"kg/m3","Water density r (typical = 1000)"]
[32,78.481012658227854,89.429423928065418,null,"D50",21.670253040365619,18.343440216943247,"mm",null,null,null,"(Pa)","(m/s)",2650,"kg/m3","Sediment density rs (typical = quartz = 2650)"]
[22.63,53.164556962025323,67.011085488349963,null,"Dg",20.232789530422835,16.625815286239149,"mm",null,null,null,40,{"$f":"SQRT(L23/N21)","v":0.2}]
[16,27.848101265822791,38.928179204335237,null,"sg",0.85959126638007455,0.86418537017698926,"f/y-units",null,null,"Depth","Slope","Shear Velocity"]
[11.31,15.189873417721525,22.82042243909541,null,"Fs",0,0,"%",null,null,"(m)",null,"(m/s)"]
[8,8.8607594936708924,13.951650893561149,null,null,null,null,null,null,null,0.5,0.01,{"$f":"SQRT(9.81*K26*L26)","v":0.22147234590350101}]
[5.66,3.7974683544303858,6.2877786634889912,null,null,null,null,null,null,null,"Depth","Slope","Shear Velocity"]
[4,1.2658227848101324,2.1858203653991097,null,null,null,null,null,null,null,"(ft)",null,"(m/s)"]
[2.83,0,0,null,null,null,null,null,null,null,1.64,0.01,{"$f":"SQRT(9.81*K29*0.3048*L29)","v":0.22144399562869163}]
[2,null,null,null,null,null,null,null,null,null,null,"Transport Rate","Unit Transport Rate"]
[1.4,null,null,null,null,null,null,null,null,null,null,"(kg/m/s)","(m2/s)"]
[1,null,null,null,null,null,null,null,null,null,null,5,{"$f":"L32/N22","v":1.8867924528301887E-3},"For bed-material load in kg/m/s, 0.2 is respectable, 1.0 is a big number, 5 is getting really big"]
[0.70699999999999996,null,null,null,null,null,null,null,null,null,"Transport Rate","Channel Width","Unit Transport Rate"]
[0.5,null,null,null,null,null,null,null,null,null,"(kg/hr)","(m)","(m2/s)"]
[0.35,null,null,null,null,null,null,null,null,null,10,10,{"$f":"K35/N22/3600/L35","v":1.0482180293501048E-7}]
[0.25,null,null,null,null,null,null,null,null,null,"Transport Rate","Channel Width","Unit Transport Rate"]
[0.17699999999999999,null,null,null,null,null,null,null,null,null,"(tons/day)","(ft)","(m2/s)"]
[null,null,null,null,null,null,null,null,null,null,10,10,{"$f":"K38*2000/2.2/N22/L38/0.3048/24/3600","v":1.3026649732438865E-5},"where ton = 2000 lb or 909 kg of sediment"]
[null,null,null,null,null,null,null,null,null,"Transport Rate","Water Discharge","Channel Width","Unit Transport Rate"]
[null,null,null,null,null,null,null,null,null,"(mg/L)","(m3/s)","(m)","(m2/s)"]
[null,null,null,null,null,null,null,null,null,1000,5,10,{"$f":"J41*K41/L41/1000/1000/2650*1000","v":1.8867924528301886E-4}]

{"sheet":"iSBTM","index":2,"n_rows":42,"n_cols":14,"rows_kept":42,"cut":false,"hidden":false,"merged":[[36,5,36,7],[37,5,37,7],[38,5,38,7],[19,9,19,12],[20,9,20,11]]}
["iSBTM - calculate bed surface grain size and bed shear velocity from"]
[null,"specified transport rate and transport grain size"]
["RULES, CONVENTIONS, AND UNITS"]
["1. Cells for input data are highlighted in GREEN, cells for output data are ORANGE"]
["2. Grain-diameters must be in millimeters (mm)"]
["3. Cumulative percentiles, not fractions, are used"]
["4. Cumulative grain-size distribution percentiles must span from 0 to 100 %"]
["5. Total transport rate must be in square-meters-per-second (m2/s)"]
["6. The 0 and 100 % must be EXACTLY 0 and 100"]
["INSTRUCTIONS"]
["1. In table below, enter grain size and cumulative % in order of decreasing grain size"]
["2. Enter your total transport rate"]
["3. Check input for errors, press Enter, and then click once on the Run iSBTM button"]
[]
["Parameter","Value","Description","Units"]
["u*",0.2,"Bed shear velocity","m/s",null,null,null,null,null,"This worksheet calculates shear velocity in units of m/s"]
["qT",3.2394888182298183E-4,"Total transport rate","m2/s",null,null,null,null,null,"as a function of transport rates per unit width in units of m2/s"]
[null,null,null,null,null,null,null,null,null,"    (m3 of solid sediment per m of channel width per s = m2/s)"]
["D (mm)","Surface CDF GSD (% Finer)","Transport CDF GSD (% Finer)",null,"Statistic","Surface GSD","Transport GSD","Units",null,"Here are some convenient unit conversions."]
[64,100,100,null,"Dmin",2.83,2.83,"mm",null,"Handy Conversion Table",null,null,null,"Input"]
[45.25,93.670886075949383,98.321066504914327,null,"Dmax",64,64,"mm",null,"From",null,null,"To","Output"]
[32,78.481012658227854,89.429423928065418,null,"D50",21.670253040365619,18.343440216943247,"mm",null,null,null,"Shear Stress","Shear Velocity",1000]
[22.63,53.164556962025316,67.011085488349963,null,"Dg",20.232789530422835,16.625815286239149,"mm",null,null,null,"(Pa)","(m/s)",2650]
[16,27.848101265822788,38.928179204335237,null,"sg",0.85959126638007466,0.86418537017698926,"f/y-units",null,null,null,49.05,{"$f":"SQRT(L24/N22)","v":0.22147234590350101}]
[11.31,15.189873417721525,22.82042243909541,null,"Fs",0,0,"%",null,null,"Depth","Slope","Shear Velocity"]
[8,8.8607594936708942,13.951650893561149,null,"Armor Ratio (D50surf / D50transport)",null,null,null,null,null,"(m)",null,"(m/s)"]
[5.66,3.7974683544303902,6.2877786634889912,null,"Convergence Stuff","Value","Units",null,null,null,0.5,0.01,{"$f":"SQRT(9.81*K27*L27)","v":0.22147234590350101}]
[4,1.2658227848101364,2.1858203653991097,null,"Maximum allowed iterations",200,"#",null,null,null,"Depth","Slope","Shear Velocity"]
[2.83,0,0,null,"Number of iterations",12,"#",null,null,null,"(ft)",null,"(m/s)"]
[2,null,null,null,"Convergence tolerance",5.0000000000000002E-5,"%",null,null,null,1.64,0.01,{"$f":"SQRT(9.81*K30*0.3048*L30)","v":0.22144399562869163}]
[1.4,null,null,null,"Relative difference in surface Dg at convergence",1.7763568394002505E-14,"%",null,null,null,null,"Transport Rate","Unit Transport Rate"]
[1,null,null,null,"Max abs error for any fraction at convergence",1.1654677223305043E-10,"%",null,null,null,null,"(kg/m/s)","(m2/s)"]
[0.70699999999999996,null,null,null,"Max abs error surface sand fraction at convergence",0,"%",null,null,null,null,1,{"$f":"L33/N23","v":3.7735849056603772E-4},"For bed-material load in kg/m/s, 0.2 is respectable, 1.0 is a big number, 5 is getting really big"]
[0.5,null,null,null,"Relative difference in u* at convergence",1.7763568394002505E-14,"%",null,null,null,"Transport Rate","Channel Width","Unit Transport Rate"]
[0.35,null,null,null,"Relative difference in qT at convergence",7.1517763087201264E-9,"%",null,null,null,"(kg/hr)","(m)","(m2/s)"]
[0.25,null,null,null,null,null,null,null,null,null,10,10,{"$f":"K36/N23/3600/L36","v":1.0482180293501048E-7}]
[0.17699999999999999,null,null,null,"Issue","Warnings",null,null,null,null,"Transport Rate","Channel Width","Unit Transport Rate"]
[null,null,null,null,"Singular Jacobian matrix","No problems",null,null,null,null,"(tons/day)","(ft)","(m2/s)"]
[null,null,null,null,"Convergence","Convergence attained, have a nice day",null,null,null,null,10,10,{"$f":"K39*2000/2.2/N23/L39/0.3048/24/3600","v":1.3026649732438865E-5},"where ton = 2000 lb or 909 kg of sediment"]
[null,null,null,null,null,null,null,null,null,"Transport Rate","Water Discharge","Channel Width","Unit Transport Rate"]
[null,null,null,null,null,null,null,null,null,"(mg/L)","(m3/s)","(m)","(m2/s)"]
[null,null,null,null,null,null,null,null,null,1000,5,10,{"$f":"J42*K42/L42/1000/1000/2650*1000","v":1.8867924528301886E-4}]

{"sheet":"STAB","index":3,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":false,"merged":[[4,9,4,11],[5,9,5,10]]}
["CHANNEL STABILITY DIAGRAM FOR GRAVEL-BED RIVERS  - INPUT WORKSHEET",null,null,null,null,"For the input entered below, here are max and min values of "]
["RULES, CONVENTIONS, AND UNITS",null,null,null,null,null,"water discharge per unit width",null,null,"This worksheet uses as input water discharge in m3/s"]
["1. Cells for input data are highlighted in GREEN",null,null,null,null,"Maximum q","Minimum q",null,null,"and transport rates in units of m3/s (m3 of solid sediment per s)"]
["2. Grain-diameters must be in millimeters (mm)",null,null,null,null,{"$f":"B16/B20","v":4},{"$f":"B16/B21","v":0.5},"Case 1",null,"Here are some convenient unit conversions."]
["3. Cumulative percentiles, not fractions, are used",null,null,null,null,{"$f":"B18/B20","v":4},{"$f":"B18/B21","v":0.5},"Case 2",null,"Handy Conversion Table",null,null,"Input"]
["4. Cumulative grain-size distribution percentiles must span from 0 to 100 %",null,null,null,null,null,null,null,null,"From",null,"To","Output"]
["5.  The 0 and 100 % must be EXACTLY 0 and 100",null,null,null,null,"For the input entered below, here are max and min values of ",null,null,null,null,"Water Discharge","Water Discharge",1000,"kg/m3","Water density r (typical = 1000)"]
["INSTRUCTIONS",null,null,null,null,null,"sediment transport rate per unit width",null,null,null,"(ft3/s)","(m3/s)",2650,"kg/m3","Sediment density rs (typical = quartz = 2650)"]
["1. In first table below, enter water discharge and sediment supply rate in units of m3/s",null,null,null,null,"Maximum qs","Minimum qs",null,null,null,1000,{"$f":"K9*(0.3048)^3","v":28.316846592000005}]
[null,"and the minimum and maximum channel widths to be evaluated",null,null,null,{"$f":"2650*B17/B20","v":2.12},{"$f":"2650*B17/B21","v":0.26500000000000001},"Case 1",null,"Transport Rate","Channel Width","Transport Rate"]
["2. In second table below, enter grain size and cumulative % in order of decreasing grain size",null,null,null,null,{"$f":"2650*B19/B20","v":2.12},{"$f":"2650*B19/B21","v":0.26500000000000001},"Case 2",null,"(kg/m/s)","(m)","(m3/s)"]
["3.  In cells to right, enter side slope angle z and side slope roughness ns",null,null,null,null,{"$f":"SQRT(1+z^2)","v":1.4142135623730951},"root",null,null,1,10,{"$f":"J12/M8*K12","v":3.7735849056603774E-3},"For bed-material load in kg/m/s, 0.2 is respectable, 1.0 is a big number, 5 is getting really big"]
["4. Check input for errors and then click once on the Run STAB button",null,null,null,null,"this cell intentionally left blank",null,null,null,null,"Transport Rate","Transport Rate"]
["5. Results appear on Worksheet \"STAB OUTPUT\"",null,null,null,null,null,null,null,null,null,"(kg/hr)","(m3/s)"]
["Parameter","Value","Description","Units","Parameter","Value","Description","Units",null,null,10,{"$f":"K15/M8/3600","v":1.0482180293501048E-6}]
["Q1",20,"Case 1 water discharge","m3/s","z",1,"side slope z:1 H:V",0,null,null,"Transport Rate","Transport Rate"]
["QT1",4.0000000000000001E-3,"Case 1 sediment supply rate","m3/s","ns",0.08,"side slope roughness","#&%@$",null,null,"(tons/day)","(m3/s)"]
["Q2",20,"Case 2 water discharge","m3/s",null,null,null,null,null,null,10,{"$f":"K18*2000/2.2/M8/24/3600","v":3.9705228384473666E-5},"where ton = 2000 lb or 909 kg of sediment"]
["QT2",4.0000000000000001E-3,"Case 2 sediment supply rate","m3/s",null,null,null,null,null,"Transport Rate","Water Discharge","Transport Rate"]
["bmin",5,"Minimum bottom width","m",null,null,null,null,null,"(mg/L)","(m3/s)","(m3/s)"]
["bmax",40,"Maximum bottom width","m",null,null,null,null,null,1000,5,{"$f":"J21*K21/1000/1000/2650*1000","v":1.8867924528301887E-3}]
[]
["D (mm)","Case 1 Transport Grain Size (% Finer)","Case 2 Transport Grain Size (% Finer)"]
[64,100,100]
[45.25,93.670886075949369,95.780590717299575]
[32,78.481012658227854,85.654008438818565]
[22.63,53.164556962025323,68.776371308016877,null,"Statistic","FIRST Transport GSD","SECOND Transport GSD","Units"]
[16,27.848101265822791,51.898734177215189,null,"Dmin",0.17699999999999999,0.17699999999999999,"mm"]
[11.31,15.189873417721525,43.459915611814345,null,"Dmax",64,64,"mm"]
[8,8.8607594936708924,39.240506329113927,null,"D50",21.670253040365619,14.798649106475827,"mm"]
[5.66,3.7974683544303858,35.864978902953588,null,"Dg",20.232789530422835,7.4694186121726753,"mm"]
[4,1.2658227848101324,34.177215189873422,null,"sg",0.85959126638007455,1.3700131291900819,"f/y-units"]
[2.83,0,32.843137254901961,null,"Fs",0,0,"%"]
[2,null,31.862745098039216]
[1.4,null,29.901960784313729]
[1,null,26.47058823529412]
[0.70699999999999996,null,19.607843137254903]
[0.5,null,11.764705882352942]
[0.35,null,5.8823529411764701]
[0.25,null,1.960784313725489]
[0.17699999999999999,null,0]

{"sheet":"STAB OUTPUT","index":4,"n_rows":22,"n_cols":18,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Channel Stability chart developed using inverse calculation of the Wilcock & Crowe (2003) transport relation.  ",null,null,null,null,null,null,null,null,null,null,"z",{"$f":"z","v":1},"side slope z:1 H:V",null,"ns",{"$f":"ns","v":0.08},"side slope roughness"]
["1. CHANNEL STABILITY DIAGRAM",null,null,null,null,null,null,null,null,null,null,"2. THRESHOLD CHECK - SLOPE AS FN(SEDIMENT SUPPLY RATE) AT MEAN WIDTH"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'STAB plot DATA'!A28","v":22.5},{"$f":"Qone/('STAB plot DATA'!A28*'STAB plot DATA'!F28)","v":2.1806173117193848},{"$f":"QTone/'STAB plot DATA'!A28*2650","v":0.47111111111111115}]
[null,null,null,null,null,null,null,null,null,null,null,"3. GRAIN-SIZE DISTRIBUTIONS",null,null,{"$f":"'STAB plot DATA'!A28","v":22.5},{"$f":"Qtwo/('STAB plot DATA'!A28*'STAB plot DATA'!N28)","v":1.7540585863354343},{"$f":"QTtwo/'STAB plot DATA'!A28*2650","v":0.47111111111111115}]

{"sheet":"STAB plot DATA","index":5,"n_rows":74,"n_cols":42,"rows_kept":74,"cut":false,"hidden":false,"merged":[[0,21,0,28],[0,29,0,36],[53,1,53,2],[54,1,54,2],[53,9,53,10],[54,9,54,10],[0,9,0,16],[55,3,55,5],[56,3,56,5],[57,3,57,5],[58,3,58,5],[0,1,0,8]]}
["OUTPUT","Case 1",null,null,null,null,null,null,null,"Case 2",null,null,null,null,null,null,null,null,null,null,"Output for different feed rates to mean width","Case 1",null,null,null,null,null,null,null,"Case 2"]
["b (m)","nD1","tb1 (Pa)","G1","Ds150","h1 (m)","nc1","Rt1 (m)","S1","nD2","tb2 (Pa)","G2","Ds250","h2 (m)","nc2","Rt2 (m)","S2",null,"QT (kg/hr)","qT (m^2/s)","b (m)","nD1","tb1 (Pa)","G1","Ds184","h1 (m)","nc1","Rt1 (m)","S1","nD2","tb2 (Pa)","G2","Ds284","h2 (m)","nc2","Rt2 (m)","S2",null,null,null,"F1","F2"]
[5,2.4990013646946193E-2,56.833088717222765,1.1736290675294265,25.229511997881453,{"$f":"IF(ISERROR(F3),B3*Qone/(SQRT(I3)*$A3),(G3*Qone/SQRT(I3)*($A3+2*F3*root)^(2/3))^0.6/($A3+z*F3))","v":1.1585164055370882},{"$f":"($A3+2*F3*root)*(($A3+z*F3)*F3/($A3+2*F3*root))^(5/3)/(($A3*F3)^(5/3)/(B3*($A3+2*F3)^(2/3))+2*F3*(1+root)/ns*(z*F3/(2*(1+root)))^(5/3))","v":3.1547829461688777E-2},{"$f":"F3*($A3+z*F3)/($A3+2*F3*root)","v":0.86201916166508707},{"$f":"IF(ISERROR(I3),0.001,(G3/B3)^1.5*C3/(9810*H3))","v":9.5327854571818429E-3},2.4643033056723305E-2,34.871736683030903,1.7169282416749714,23.199298246445885,{"$f":"IF(ISERROR(N3),J3*Qtwo/(SQRT(Q3)*$A3),(O3*Qtwo/SQRT(Q3)*($A3+2*N3*root)^(2/3))^0.6/($A3+z*N3))","v":1.3883038730619899},{"$f":"($A3+2*N3*root)*(($A3+z*N3)*N3/($A3+2*N3*root))^(5/3)/(($A3*N3)^(5/3)/(J3*($A3+2*N3)^(2/3))+2*N3*(1+root)/ns*(z*N3/(2*(1+root)))^(5/3))","v":3.2509178402167896E-2},{"$f":"N3*($A3+z*N3)/($A3+2*N3*root)","v":0.99352401033704973},{"$f":"IF(ISERROR(Q3),0.001,(O3/J3)^1.5*K3/(9810*P3))","v":5.4211815730635772E-3},null,{"$f":"T3*U3*2650*3600","v":2.1465000000000001},1E-8,22.5,2.6354470764625052E-2,12.506263521352809,1.5824234302437479,32.016840212131491,{"$f":"IF(ISERROR(Z3),V3*Qone/(SQRT(AC3)*$U3),(AA3*Qone/SQRT(AC3)*($U3+2*Z3*root)^(2/3))^0.6/($U3+z*Z3))","v":0.68872653018469121},{"$f":"($U3+2*Z3*root)*(($U3+z*Z3)*Z3/($U3+2*Z3*root))^(5/3)/(($U3*Z3)^(5/3)/(V3*($U3+2*Z3)^(2/3))+2*Z3*(1+root)/ns*(z*Z3/(2*(1+root)))^(5/3))","v":2.7179984174732868E-2},{"$f":"Z3*($U3+z*Z3)/($U3+2*Z3*root)","v":0.65325109625507238},{"$f":"IF(ISERROR(AC3),0.001,(AA3/V3)^1.5*W3/(9810*AB3))","v":2.0439523694839165E-3},2.641473549979835E-2,10.72000306630774,4.1251810509726088,30.812704120716841,{"$f":"IF(ISERROR(AH3),AD3*Qtwo/(SQRT(AK3)*$U3),(AI3*Qtwo/SQRT(AK3)*($U3+2*AH3*root)^(2/3))^0.6/($U3+z*AH3))","v":0.73659631462838926},{"$f":"($U3+2*AH3*root)*(($U3+z*AH3)*AH3/($U3+2*AH3*root))^(5/3)/(($U3*AH3)^(5/3)/(AD3*($U3+2*AH3)^(2/3))+2*AH3*(1+root)/ns*(z*AH3/(2*(1+root)))^(5/3))","v":2.7300747654108604E-2},{"$f":"AH3*($U3+z*AH3)/($U3+2*AH3*root)","v":0.69624156732903897},{"$f":"IF(ISERROR(AK3),0.001,(AI3/AD3)^1.5*AE3/(9810*AJ3))","v":1.6491431897958258E-3},null,null,null,{"$f":"Qone/(A3*SQRT(9.81)*F3^1.5)","v":1.0241703657914945},{"$f":"Qtwo/(A3*SQRT(9.81)*N3^1.5)","v":0.78072607575597264}]
[5.7,2.5011753007736042E-2,54.808244466380351,1.1800463723446928,25.361484956077152,{"$f":"IF(ISERROR(F4),B4*Qone/(SQRT(I4)*$A4),(G4*Qone/SQRT(I4)*($A4+2*F4*root)^(2/3))^0.6/($A4+z*F4))","v":1.0694936489677855},{"$f":"($A4+2*F4*root)*(($A4+z*F4)*F4/($A4+2*F4*root))^(5/3)/(($A4*F4)^(5/3)/(B4*($A4+2*F4)^(2/3))+2*F4*(1+root)/ns*(z*F4/(2*(1+root)))^(5/3))","v":3.024954044206269E-2},{"$f":"F4*($A4+z*F4)/($A4+2*F4*root)","v":0.82979289840441828},{"$f":"IF(ISERROR(I4),0.001,(G4/B4)^1.5*C4/(9810*H4))","v":8.9550733043455635E-3},2.4685548023042674E-2,33.470412998379921,1.7510420841271008,23.440481524609577,1.2883602395360991,{"$f":"($A4+2*N4*root)*(($A4+z*N4)*N4/($A4+2*N4*root))^(5/3)/(($A4*N4)^(5/3)/(J4*($A4+2*N4)^(2/3))+2*N4*(1+root)/ns*(z*N4/(2*(1+root)))^(5/3))","v":3.1005473690950143E-2},0.9635588215465607,4.9843350544767438E-3,null,3.8478639816000002,1.7926224E-8,22.5,2.6354470764625052E-2,13.344214053983732,1.5824234302437485,32.016840212131505,0.67005931550485176,2.7157129280087421E-2,0.63640819553071604,{"$f":"IF(ISERROR(AC4),0.001,(AA4/V4)^1.5*W4/(9810*AB4))","v":2.2357980303448735E-3},2.641473549979835E-2,11.438269738354169,4.1251810509726115,30.812704120716859,0.71664718955618567,2.7276207547547268E-2,0.6783608095480862,1.8035872514207726E-3,null,null,null,1.0128690983193194,0.76606331610188949]
[6.4,2.5031534361482623E-2,53.119121142411643,1.1858926941054895,25.48207086274174,{"$f":"IF(ISERROR(F5),B5*Qone/(SQRT(I5)*$A5),(G5*Qone/SQRT(I5)*($A5+2*F5*root)^(2/3))^0.6/($A5+z*F5))","v":0.9939279965960609},{"$f":"($A5+2*F5*root)*(($A5+z*F5)*F5/($A5+2*F5*root))^(5/3)/(($A5*F5)^(5/3)/(B5*($A5+2*F5)^(2/3))+2*F5*(1+root)/ns*(z*F5/(2*(1+root)))^(5/3))","v":2.9316325600711467E-2},{"$f":"F5*($A5+z*F5)/($A5+2*F5*root)","v":0.7978319687814539},8.6020811831680633E-3,2.4723744114932687E-2,32.312186962061979,1.782120233356451,23.65894262518858,1.2024912314202159,2.9917386526664595E-2,0.93273960907605713,4.700575629645252E-3,null,6.8977671655693467,3.2134950689817597E-8,22.5,2.6354470764625052E-2,14.238309341116071,1.5824234302437479,32.016840212131491,0.65189254560725229,2.7134911062045412E-2,0.61997417090812579,2.4458339831661445E-3,2.641475169352421E-2,12.204444528687716,4.1251483356581362,30.812459756338015,0.69723768238188921,2.7252374894947289E-2,0.6609157983920606,1.9726026411640281E-3,null,null,null,1.0068925609822945,0.75664582612536424]
[7.1,2.5049721994972522E-2,51.681274576653493,1.1912727674233923,25.59336277979838,{"$f":"IF(ISERROR(F6),B6*Qone/(SQRT(I6)*$A6),(G6*Qone/SQRT(I6)*($A6+2*F6*root)^(2/3))^0.6/($A6+z*F6))","v":0.92904806750197189},{"$f":"($A6+2*F6*root)*(($A6+z*F6)*F6/($A6+2*F6*root))^(5/3)/(($A6*F6)^(5/3)/(B6*($A6+2*F6)^(2/3))+2*F6*(1+root)/ns*(z*F6/(2*(1+root)))^(5/3))","v":2.8624333879183155E-2},{"$f":"F6*($A6+z*F6)/($A6+2*F6*root)","v":0.76681407452471251},8.3921425206182135E-3,2.4758460491825625E-2,31.334575035807536,1.8107115837488696,23.858970938739102,1.1280261973291683,2.9106897224855533E-2,0.9019380128300768,4.5142595446624042E-3,null,12.36509193098412,5.7605832429462472E-8,22.5,2.6354470764625052E-2,15.192311219917153,1.5824234302437485,32.016840212131505,0.63421309483500565,2.7113311667248237E-2,0.60394032513271723,2.6757973115511535E-3,2.6415011392770381E-2,13.018234523177854,4.1246123765217497,30.808456453189329,0.67843500919421751,2.7229563520981111E-2,0.64397082604180345,2.1567594374520935E-3,null,null,null,1.0043379350142692,0.75068608293030659]
[7.8,2.5066584180546803E-2,50.437380869731527,1.1962639754374353,25.69690571213394,{"$f":"IF(ISERROR(F7),B7*Qone/(SQRT(I7)*$A7),(G7*Qone/SQRT(I7)*($A7+2*F7*root)^(2/3))^0.6/($A7+z*F7))","v":0.87276226336850937},{"$f":"($A7+2*F7*root)*(($A7+z*F7)*F7/($A7+2*F7*root))^(5/3)/(($A7*F7)^(5/3)/(B7*($A7+2*F7)^(2/3))+2*F7*(1+root)/ns*(z*F7/(2*(1+root)))^(5/3))","v":2.8097749347527307E-2},{"$f":"F7*($A7+z*F7)/($A7+2*F7*root)","v":0.73713072507347255},8.2775835095640921E-3,2.4790309021975206E-2,30.495444850859201,1.8372234496897597,24.043712888706732,1.062884642894204,2.8488356978154789E-2,0.87173511438891649,{"$f":"IF(ISERROR(Q7),0.001,(O7/J7)^1.5*K7/(9810*P7))","v":4.3929839726244199E-3},null,22.165940773541386,1.0326550558370084E-7,22.5,2.6354470764625052E-2,16.210233579932094,1.5824234302437468,32.01684021213147,0.61700816657955559,2.7092313742776174E-2,0.58829808818621721,2.9275918116714039E-3,2.6416254373318678E-2,13.868546745487636,4.1219570868400304,30.788622983019984,0.66051240310127868,2.7208864721593271E-2,0.62777713065005092,2.3540475542471518E-3,null,null,null,1.0040537197825172,0.74708788015766014]
[8.5,2.5082324645175163E-2,49.346960984743021,1.2009252561625319,25.793875465683456,{"$f":"IF(ISERROR(F8),B8*Qone/(SQRT(I8)*$A8),(G8*Qone/SQRT(I8)*($A8+2*F8*root)^(2/3))^0.6/($A8+z*F8))","v":0.82347481380404097},{"$f":"($A8+2*F8*root)*(($A8+z*F8)*F8/($A8+2*F8*root))^(5/3)/(($A8*F8)^(5/3)/(B8*($A8+2*F8)^(2/3))+2*F8*(1+root)/ns*(z*F8/(2*(1+root)))^(5/3))","v":2.7688203147749481E-2},{"$f":"F8*($A8+z*F8)/($A8+2*F8*root)","v":0.70898037608150455},8.2290115540659785E-3,2.4819749966146269E-2,29.765225734828256,1.8619670250339058,24.215548084957401,1.0054390435651201,2.8006520797671124E-2,0.84249812408443125,4.3168192854043117E-3,null,39.735161947723611,1.851160584566672E-7,22.5,2.6354470764625052E-2,17.296359251215442,1.5824234302437479,32.016840212131491,0.60026528582229133,2.7071900422555677E-2,0.57303901812864155,3.2033040479984864E-3,2.641983304774749E-2,14.724191796007366,4.1140227741817297,30.729358280375273,0.64403510421723753,2.7192352475297627E-2,0.61285306738854994,2.5572969616601583E-3,null,null,null,1.0053125060936774,0.74514869880495982]
[9.1999999999999993,2.5097102025896888E-2,48.38049846469373,1.2053026253986319,25.885189435814773,{"$f":"IF(ISERROR(F9),B9*Qone/(SQRT(I9)*$A9),(G9*Qone/SQRT(I9)*($A9+2*F9*root)^(2/3))^0.6/($A9+z*F9))","v":0.77995332034699427},{"$f":"($A9+2*F9*root)*(($A9+z*F9)*F9/($A9+2*F9*root))^(5/3)/(($A9*F9)^(5/3)/(B9*($A9+2*F9)^(2/3))+2*F9*(1+root)/ns*(z*F9/(2*(1+root)))^(5/3))","v":2.736372567964801E-2},{"$f":"F9*($A9+z*F9)/($A9+2*F9*root)","v":0.68243640735947564},8.2274759395236825E-3,2.4847139103913344E-2,29.122475753675651,1.8851861913737262,24.376325393965843,0.95440671214939332,2.7624548431392136E-2,0.81444249703895766,4.2729425372537494E-3,null,71.230141375116972,3.3184319298913106E-7,22.5,2.6354470764625052E-2,18.45525802400925,1.5824234302437479,32.016840212131491,0.5839722918041006,2.7052055314086314E-2,0.55815480179128463,3.5052209590926229E-3,2.6426992023392808E-2,15.546968084013775,4.097813507059298,30.608284478841306,0.62950166167674071,2.7181903586708741E-2,0.59966063238650869,2.7568895192144841E-3,null,null,null,1.0076384884469056,0.74440183866156362]
[9.9,2.5111042451273383E-2,47.51588937406401,1.2094327581036477,25.971578378405415,{"$f":"IF(ISERROR(F10),B10*Qone/(SQRT(I10)*$A10),(G10*Qone/SQRT(I10)*($A10+2*F10*root)^(2/3))^0.6/($A10+z*F10))","v":0.74123417551267268},{"$f":"($A10+2*F10*root)*(($A10+z*F10)*F10/($A10+2*F10*root))^(5/3)/(($A10*F10)^(5/3)/(B10*($A10+2*F10)^(2/3))+2*F10*(1+root)/ns*(z*F10/(2*(1+root)))^(5/3))","v":2.7102530744349939E-2},{"$f":"F10*($A10+z*F10)/($A10+2*F10*root)","v":0.657494168152846},8.2602959089214702E-3,2.4872757255389941E-2,28.551220637143672,1.9070758559559082,24.527510987612882,0.90876773338851213,2.7317152144114887E-2,0.7876790241174908,4.2527869592871607E-3,null,127.6887469842015,5.948695410398393E-7,22.5,2.6354513062445021E-2,19.691230946653882,1.5823306266656163,32.014962536867486,0.56812514539720094,2.7032815246247788E-2,0.54364441888344306,3.8356886224864338E-3,2.6438951343139241E-2,16.304161081591275,4.070497150319504,30.404247175392342,0.61716991556731149,2.7179072814894959E-2,0.58844532449921094,2.9438044053916126E-3,null,null,null,1.010711355727826,0.74452785293783186]
[10.6,2.5124247985446237E-2,46.736204466202302,1.2133453980922253,26.053634658215017,{"$f":"IF(ISERROR(F11),B11*Qone/(SQRT(I11)*$A11),(G11*Qone/SQRT(I11)*($A11+2*F11*root)^(2/3))^0.6/($A11+z*F11))","v":0.70655484441660066},{"$f":"($A11+2*F11*root)*(($A11+z*F11)*F11/($A11+2*F11*root))^(5/3)/(($A11*F11)^(5/3)/(B11*($A11+2*F11)^(2/3))+2*F11*(1+root)/ns*(z*F11/(2*(1+root)))^(5/3))","v":2.6889371324298479E-2},{"$f":"F11*($A11+z*F11)/($A11+2*F11*root)","v":0.63410246067743203},8.318717180265018E-3,2.4896830207233149E-2,28.039284628914643,1.9277945022359477,24.670288908283659,0.86770354395508309,2.7066529682354883E-2,0.76224811802133063,4.2504444009257491E-3,null,228.89770807181208,1.0663764643457352E-6,22.5,2.6354749928755611E-2,21.004406139472064,1.5813708898485594,31.995544383843377,0.5527697752551568,2.7014390103499368E-2,0.52955267396693351,4.1960111683548053E-3,2.6457557754018028E-2,16.958008885974415,4.0269344000296075,30.078858757579553,0.6073239829332564,2.718608926195161E-2,0.57947660306997806,3.1071729260115141E-3,null,null,null,1.0143102379446542,0.74530248600043503]
[11.3,2.5136802475095775E-2,46.028226070528333,1.2170650304750492,26.131845709144727,{"$f":"IF(ISERROR(F12),B12*Qone/(SQRT(I12)*$A12),(G12*Qone/SQRT(I12)*($A12+2*F12*root)^(2/3))^0.6/($A12+z*F12))","v":0.67530499960626211},{"$f":"($A12+2*F12*root)*(($A12+z*F12)*F12/($A12+2*F12*root))^(5/3)/(($A12*F12)^(5/3)/(B12*($A12+2*F12)^(2/3))+2*F12*(1+root)/ns*(z*F12/(2*(1+root)))^(5/3))","v":2.6713324713831976E-2},{"$f":"F12*($A12+z*F12)/($A12+2*F12*root)","v":0.61218411278576901},8.3965338190076788E-3,2.4919542359064906E-2,27.577204181750343,1.9474728985220384,24.805630179044723,0.83055105485461722,2.6859866315518354E-2,0.73814410880401826,4.261728177422674E-3,null,410.32715879819114,1.9116103368189664E-6,22.5,2.6354137523078216E-2,22.385535495887623,1.5773608982252481,31.914411067310159,0.53801111313899141,2.6995839109639087E-2,0.51597901012401992,4.5849909244237205E-3,2.6483977978103319E-2,17.455038374351286,3.9559904641708692,29.548948802655513,0.60043438796759252,2.7204715650712915E-2,0.57319331660758799,3.2317826263560802E-3,null,null,null,1.0182797352111468,0.74656486509620612]
[12,2.5148775707321269E-2,45.381461287394814,1.220612073528994,26.206617862931253,{"$f":"IF(ISERROR(F13),B13*Qone/(SQRT(I13)*$A13),(G13*Qone/SQRT(I13)*($A13+2*F13*root)^(2/3))^0.6/($A13+z*F13))","v":0.64699089985519154},{"$f":"($A13+2*F13*root)*(($A13+z*F13)*F13/($A13+2*F13*root))^(5/3)/(($A13*F13)^(5/3)/(B13*($A13+2*F13)^(2/3))+2*F13*(1+root)/ns*(z*F13/(2*(1+root)))^(5/3))","v":2.6566402990361535E-2},{"$f":"F13*($A13+z*F13)/($A13+2*F13*root)","v":0.59164915239041471},8.4892453424828679E-3,2.4941046361343474E-2,27.157498429212179,1.9662203221382175,24.934341794008585,0.79676826837491077,2.6687753657042519E-2,0.7153321400375765,4.2836013137862285E-3,null,735.56165618999455,3.4267955098532236E-6,22.5,2.6343036366164065E-2,23.812999365571201,1.5657744577370394,31.679985055505462,0.52388123229506933,2.6967360048962007E-2,0.50295638555043631,4.9988910321630961E-3,2.6504622994136463E-2,17.750138808396006,3.8373456412008102,28.66274095372502,0.59657275958429978,2.7221125983459649E-2,0.56966881384221524,3.3058792224333997E-3,null,null,null,1.0225086428414727,0.74819741126431871]
[12.7,2.5160226435137531E-2,44.787458348114676,1.2240037477125363,26.278293711953278,{"$f":"IF(ISERROR(F14),B14*Qone/(SQRT(I14)*$A14),(G14*Qone/SQRT(I14)*($A14+2*F14*root)^(2/3))^0.6/($A14+z*F14))","v":0.62120913238884845},{"$f":"($A14+2*F14*root)*(($A14+z*F14)*F14/($A14+2*F14*root))^(5/3)/(($A14*F14)^(5/3)/(B14*($A14+2*F14)^(2/3))+2*F14*(1+root)/ns*(z*F14/(2*(1+root)))^(5/3))","v":2.6442656407655845E-2},{"$f":"F14*($A14+z*F14)/($A14+2*F14*root)","v":0.57240306748512049},8.5935233681351079E-3,2.4961470084630465E-2,26.774165813725602,1.9841291098329432,25.057102267549105,0.76590834791383766,2.6543161588188924E-2,0.69375974876078705,4.3138156338289038E-3,null,1318.5843014672826,6.142950391182309E-6,22.5,2.6287891030111869E-2,25.272970637407514,1.5410881619137835,31.180512427827768,0.50989531403351984,2.6894143855495382E-2,0.4900400525361584,5.4401224381496966E-3,2.6463534449315748E-2,17.87747507628837,3.6543170982953046,27.295624148787791,0.59398425691720724,2.7175895505274685E-2,0.56730519910013077,3.3429080760891761E-3,null,null,null,1.0269162436264752,0.75011278276720506]
[13.4,2.5171204623579524E-2,44.239321808390386,1.2272547220331838,26.347165016020121,{"$f":"IF(ISERROR(F15),B15*Qone/(SQRT(I15)*$A15),(G15*Qone/SQRT(I15)*($A15+2*F15*root)^(2/3))^0.6/($A15+z*F15))","v":0.59762703565909248},{"$f":"($A15+2*F15*root)*(($A15+z*F15)*F15/($A15+2*F15*root))^(5/3)/(($A15*F15)^(5/3)/(B15*($A15+2*F15)^(2/3))+2*F15*(1+root)/ns*(z*F15/(2*(1+root)))^(5/3))","v":2.6337580151371213E-2},{"$f":"F15*($A15+z*F15)/($A15+2*F15*root)","v":0.55435184674058713},8.7068639764025201E-3,2.4980921763897677E-2,26.422328471144013,2.0012780509101074,25.174487961362598,0.73759991120416168,2.6420753574784295E-2,0.67336469822405876,4.3506770539636121E-3,null,2363.7237550986038,1.101199047332217E-5,22.5,2.6155560540839225E-2,26.794668147765723,1.5017134432635568,30.383852032558117,0.49525522277172235,2.6741505498897675E-2,0.47649130731162581,5.9259383058798609E-3,2.6332922920614711E-2,17.972979784502755,3.414306388342554,25.502883684745939,0.59016171021063235,2.7037536427675202E-2,0.56381314871616872,3.3807881158773503E-3,null,null,null,1.0314432535570033,0.75224517355490894]
[14.1,2.5181753146886848E-2,43.731361609884395,1.2303776033171931,26.413482466994388,{"$f":"IF(ISERROR(F16),B16*Qone/(SQRT(I16)*$A16),(G16*Qone/SQRT(I16)*($A16+2*F16*root)^(2/3))^0.6/($A16+z*F16))","v":0.57596793822916792},{"$f":"($A16+2*F16*root)*(($A16+z*F16)*F16/($A16+2*F16*root))^(5/3)/(($A16*F16)^(5/3)/(B16*($A16+2*F16)^(2/3))+2*F16*(1+root)/ns*(z*F16/(2*(1+root)))^(5/3))","v":2.6247712880273943E-2},{"$f":"F16*($A16+z*F16)/($A16+2*F16*root)","v":0.53740493406167145},8.8273551412373415E-3,2.4999493865116913E-2,26.097975734110157,2.0177349617822755,25.286992934686733,0.71153192723242087,2.6316420731941546E-2,0.65408020228497366,4.3928888915460047E-3,null,4237.2641508018714,1.9740340791063925E-5,22.5,2.5963998208355384E-2,28.475387166389904,1.4506047096715848,29.349779782625298,0.47960767410916061,2.652746442130903E-2,0.46197807119361628,6.4888169726146803E-3,2.6118759779252192E-2,18.197400078135878,3.1344962098952043,23.412864329975946,0.58301057584375116,2.6809683661965417E-2,0.55727515247157045,3.4616197845435291E-3,null,null,null,1.036045708802062,0.75454438412513236]
[14.8,2.5191909091158173E-2,43.258834377183717,1.2333833123713382,26.477463192394698,{"$f":"IF(ISERROR(F17),B17*Qone/(SQRT(I17)*$A17),(G17*Qone/SQRT(I17)*($A17+2*F17*root)^(2/3))^0.6/($A17+z*F17))","v":0.55599990753873463},{"$f":"($A17+2*F17*root)*(($A17+z*F17)*F17/($A17+2*F17*root))^(5/3)/(($A17*F17)^(5/3)/(B17*($A17+2*F17)^(2/3))+2*F17*(1+root)/ns*(z*F17/(2*(1+root)))^(5/3))","v":2.6170359482762365E-2},{"$f":"F17*($A17+z*F17)/($A17+2*F17*root)","v":0.52147684587244614},8.9535175124716374E-3,2.5017265897677606E-2,25.797775681550355,2.0335585817402735,25.39504329328264,0.68744203830475814,2.6226958352499045E-2,0.63583834747602752,4.4394448085550257E-3,null,7595.8146314444111,3.5386977085694908E-5,22.5,2.5746559710149414E-2,30.440223715854849,1.3926398484766815,28.176988945908647,0.46287237017051275,2.6286032682827743E-2,0.44641898163155952,7.1704256346133552E-3,2.585234257331254E-2,18.747309389350889,2.8459266322269769,21.257417355634082,0.57070537690822942,2.6522321907379562E-2,0.54600925551734525,3.6369505337067952E-3,null,null,null,1.0406907574561504,0.75697170607451181]
[15.5,2.5201704768274869E-2,42.817749583098177,1.2362813772326069,26.539296602465779,{"$f":"IF(ISERROR(F18),B18*Qone/(SQRT(I18)*$A18),(G18*Qone/SQRT(I18)*($A18+2*F18*root)^(2/3))^0.6/($A18+z*F18))","v":0.53752708456652154},{"$f":"($A18+2*F18*root)*(($A18+z*F18)*F18/($A18+2*F18*root))^(5/3)/(($A18*F18)^(5/3)/(B18*($A18+2*F18)^(2/3))+2*F18*(1+root)/ns*(z*F18/(2*(1+root)))^(5/3))","v":2.6103396064037186E-2},{"$f":"F18*($A18+z*F18)/($A18+2*F18*root)","v":0.5064879420311944},9.0841931547736218E-3,2.5034307227806425E-2,25.518934453587384,2.048800450986509,25.499012200647694,0.66510746955275912,2.6149838113832195E-2,0.61857229482128218,4.4895540545634169E-3,null,13616.427454575,6.3435487792103413E-5,22.5,2.5557612496000071E-2,33.00447313384722,1.339896429607633,27.109842452816256,0.44442953036577143,2.6071902826326838E-2,0.42922786367185367,8.0759674836330311E-3,2.5593423488141524E-2,19.860939901612042,2.5823739008829318,19.288831678843927,0.55215827234183112,2.6235494580832547E-2,0.52899084540330554,3.9721344742641362E-3,null,null,null,1.0453537118433356,0.7594969880846969]
[16.2,2.5211168515077577E-2,42.404722180836487,1.2390801646551624,26.5991490038701,{"$f":"IF(ISERROR(F19),B19*Qone/(SQRT(I19)*$A19),(G19*Qone/SQRT(I19)*($A19+2*F19*root)^(2/3))^0.6/($A19+z*F19))","v":0.52038294405102226},{"$f":"($A19+2*F19*root)*(($A19+z*F19)*F19/($A19+2*F19*root))^(5/3)/(($A19*F19)^(5/3)/(B19*($A19+2*F19)^(2/3))+2*F19*(1+root)/ns*(z*F19/(2*(1+root)))^(5/3))","v":2.604513046248217E-2},{"$f":"F19*($A19+z*F19)/($A19+2*F19*root)","v":0.49236467043910981},9.2184663568756261E-3,2.505067813807008E-2,25.259089526999905,2.0635056763349797,25.599224701718601,0.64433785618281791,2.608304335841348E-2,0.60221761819385722,4.5425884509210559E-3,null,24409.112863046121,1.1371587637105112E-4,22.5,2.5394657664463059E-2,36.350682188399354,1.2929820631527313,26.160633950381101,0.42422611401920102,2.5882457566563509E-2,0.41034174735396367,9.2916443190205807E-3,2.5350961808147623E-2,21.63131334889297,2.3435944140853322,17.505287735952898,0.52820897563287028,2.5959544037351678E-2,0.50694783581074432,4.5071762004487877E-3,null,null,null,1.0500159514216911,0.76209656781376112]
[16.899999999999999,2.5220325330479337E-2,42.01685907637858,1.2417870649178204,26.657167281631327,{"$f":"IF(ISERROR(F20),B20*Qone/(SQRT(I20)*$A20),(G20*Qone/SQRT(I20)*($A20+2*F20*root)^(2/3))^0.6/($A20+z*F20))","v":0.50442500338649399},{"$f":"($A20+2*F20*root)*(($A20+z*F20)*F20/($A20+2*F20*root))^(5/3)/(($A20*F20)^(5/3)/(B20*($A20+2*F20)^(2/3))+2*F20*(1+root)/ns*(z*F20/(2*(1+root)))^(5/3))","v":2.5994200949835244E-2},{"$f":"F20*($A20+z*F20)/($A20+2*F20*root)","v":0.47903949296523091},9.3556063275456701E-3,2.5066431714151762E-2,25.016227829319991,2.0777141994948591,25.695967924606087,0.62496958234134359,2.6024950184786243E-2,0.58671309886004941,4.5980439633131268E-3,null,43756.322482424606,2.0384962721837693E-4,22.5,2.5253401429330281E-2,40.705446787556575,1.2515541357473592,25.322431414506568,0.402367256388655,2.5713437398144717E-2,0.38984418173718249,1.0935857544722479E-2,2.5122637632193121E-2,24.203936253259268,2.1288632957675078,15.901371124177086,0.49972780113089743,2.5693258553362516E-2,0.48063355325894536,5.3092580828572713E-3,null,null,null,1.0546634098091003,0.76475172742945052]
[17.600000000000001,2.5229197388650836E-2,41.651670616886427,1.2444086408860593,26.713481867879548,{"$f":"IF(ISERROR(F21),B21*Qone/(SQRT(I21)*$A21),(G21*Qone/SQRT(I21)*($A21+2*F21*root)^(2/3))^0.6/($A21+z*F21))","v":0.48953063221242377},{"$f":"($A21+2*F21*root)*(($A21+z*F21)*F21/($A21+2*F21*root))^(5/3)/(($A21*F21)^(5/3)/(B21*($A21+2*F21)^(2/3))+2*F21*(1+root)/ns*(z*F21/(2*(1+root)))^(5/3))","v":2.594950162698112E-2},{"$f":"F21*($A21+z*F21)/($A21+2*F21*root)","v":0.46645062657085928},9.4950251050716569E-3,2.5081614880836503E-2,24.788622038933482,2.0914615216138435,25.789496379264339,0.60686124861277113,2.5974239154931803E-2,0.57200112958545013,4.6555125483719473E-3,null,78438.563823617966,3.6542540798331218E-4,22.5,2.5130532851262516E-2,46.377858610406804,1.2152075048351103,24.587037681119078,0.37905049713569661,2.5561689491957525E-2,0.36790567314991185,1.3182172389268873E-2,2.4908221171190043E-2,27.805062546822018,1.9376481347080983,14.473105041230337,0.46769582338602728,2.5437641374094683E-2,0.45090735644140328,6.487371051280692E-3,null,null,null,1.0592854693561951,0.76744756890992194]
[18.3,2.5237804456295986E-2,41.307000825245403,1.2469507493728524,26.768209158116946,{"$f":"IF(ISERROR(F22),B22*Qone/(SQRT(I22)*$A22),(G22*Qone/SQRT(I22)*($A22+2*F22*root)^(2/3))^0.6/($A22+z*F22))","v":0.4755937061937085},{"$f":"($A22+2*F22*root)*(($A22+z*F22)*F22/($A22+2*F22*root))^(5/3)/(($A22*F22)^(5/3)/(B22*($A22+2*F22)^(2/3))+2*F22*(1+root)/ns*(z*F22/(2*(1+root)))^(5/3))","v":2.5910126770072307E-2},{"$f":"F22*($A22+z*F22)/($A22+2*F22*root)","v":0.45454168526177313},9.6362462192016579E-3,2.5096269329283844E-2,24.574780521031698,2.1047793494015261,25.880036795864005,0.58989002701008575,2.5929829367628873E-2,0.55802787027356859,4.7146611961507183E-3,null,140610.72653404719,6.5506977188002418E-4,22.5,2.5023444832683487E-2,53.793328267993296,1.1835011367408799,23.945529408694398,0.35455236597457118,2.5424865334753487E-2,0.34477282761704769,1.6288973808856213E-2,2.4708179569394535E-2,32.773263415336132,1.7694077479323511,13.216447164928441,0.43313050806695241,2.5194393839950379E-2,0.41867253022509093,8.216199230997449E-3,null,null,null,1.0638741442049826,0.77017217013500583]
[19,2.5246164234883142E-2,40.980971857906916,1.249418640796937,26.821453494800547,{"$f":"IF(ISERROR(F23),B23*Qone/(SQRT(I23)*$A23),(G23*Qone/SQRT(I23)*($A23+2*F23*root)^(2/3))^0.6/($A23+z*F23))","v":0.462521914064288},{"$f":"($A23+2*F23*root)*(($A23+z*F23)*F23/($A23+2*F23*root))^(5/3)/(($A23*F23)^(5/3)/(B23*($A23+2*F23)^(2/3))+2*F23*(1+root)/ns*(z*F23/(2*(1+root)))^(5/3))","v":2.5875328818972695E-2},{"$f":"F23*($A23+z*F23)/($A23+2*F23*root)","v":0.44326127697316908},9.778881068705586E-3,2.511043227501257E-2,24.373407575330315,2.1176961265551366,25.96779208925572,0.57394870738531367,2.5890828594866799E-2,0.54474324125147466,4.7752161377034681E-3,null,252061.93806520733,1.1742927466350213E-3,22.5,2.4930043703771814E-2,63.542178288088451,1.1559819296938401,23.388739084467513,0.32921133428150035,2.5301205596122853E-2,0.32075399790883219,2.0646587307311851E-2,2.4517982742091961E-2,39.602761438847317,1.6232177195630682,12.124492646112868,0.39698817595027619,2.4960016238890763E-2,0.38478984343648404,1.0776383911012122E-2,null,null,null,1.0684234702626918,0.77291594693502419]
[19.7,2.5254292643564782E-2,40.671939378068615,1.2518170416671992,26.873308808648289,{"$f":"IF(ISERROR(F24),B24*Qone/(SQRT(I24)*$A24),(G24*Qone/SQRT(I24)*($A24+2*F24*root)^(2/3))^0.6/($A24+z*F24))","v":0.45023457447998999},{"$f":"($A24+2*F24*root)*(($A24+z*F24)*F24/($A24+2*F24*root))^(5/3)/(($A24*F24)^(5/3)/(B24*($A24+2*F24)^(2/3))+2*F24*(1+root)/ns*(z*F24/(2*(1+root)))^(5/3))","v":2.5844486314968069E-2},{"$f":"F24*($A24+z*F24)/($A24+2*F24*root)","v":0.43256258894354804},9.9226109126990675E-3,2.5124137082548126E-2,24.183371577224506,2.1302374742700105,26.052944633572913,0.5589432880704952,2.5856495163018481E-2,0.53210081440122914,4.8369508065187654E-3,null,451851.87636310339,2.105063481775464E-3,22.5,2.484861500577942E-2,76.449749556726545,1.132203852027442,22.907642243605231,0.30340761530104615,2.5189379628644176E-2,0.29620165503807727,2.6852981048863935E-2,2.4307647648259503E-2,49.007214078931185,1.4975989199245265,11.186193246053955,0.35990335362823045,2.4704806379008366E-2,0.34983288252743611,1.4631476766800154E-2,null,null,null,1.0729290453844686,0.77567116595873542]
[20.399999999999999,2.5262204054783619E-2,40.378456393876085,1.2541502233511226,26.923859986672745,{"$f":"IF(ISERROR(F25),B25*Qone/(SQRT(I25)*$A25),(G25*Qone/SQRT(I25)*($A25+2*F25*root)^(2/3))^0.6/($A25+z*F25))","v":0.4386608539257324},{"$f":"($A25+2*F25*root)*(($A25+z*F25)*F25/($A25+2*F25*root))^(5/3)/(($A25*F25)^(5/3)/(B25*($A25+2*F25)^(2/3))+2*F25*(1+root)/ns*(z*F25/(2*(1+root)))^(5/3))","v":2.5817079182104012E-2},{"$f":"F25*($A25+z*F25)/($A25+2*F25*root)","v":0.42240298178401553},1.0067172998717346E-2,2.5137413784052303E-2,24.003679225439164,2.1424265590244165,26.135658987132366,0.54479099797421415,2.5826208522415701E-2,0.52005764300187052,4.8996765635818378E-3,null,809999.79505052953,3.7735839508526883E-3,22.5,2.4777726148829615E-2,93.677923460603168,1.1117415369197607,22.493632528726327,0.27754087410960088,2.5088361028992489E-2,0.27149226889517708,3.5836620188759424E-2,2.4122144462501292E-2,62.015171894097584,1.3906315427578164,10.387209128149635,0.32343441613170915,2.447616979730851E-2,0.31526559350635347,2.0494799914906752E-2,null,null,null,1.0773876798116344,0.77843156924672441]
[21.1,2.5269911491812073E-2,40.099243725266952,1.2564220597953655,26.973184020166517,{"$f":"IF(ISERROR(F26),B26*Qone/(SQRT(I26)*$A26),(G26*Qone/SQRT(I26)*($A26+2*F26*root)^(2/3))^0.6/($A26+z*F26))","v":0.4277383025214257},{"$f":"($A26+2*F26*root)*(($A26+z*F26)*F26/($A26+2*F26*root))^(5/3)/(($A26*F26)^(5/3)/(B26*($A26+2*F26)^(2/3))+2*F26*(1+root)/ns*(z*F26/(2*(1+root)))^(5/3))","v":2.5792669489719408E-2},{"$f":"F26*($A26+z*F26)/($A26+2*F26*root)","v":0.41274360382387343},1.0212349775013297E-2,2.5150289512918225E-2,23.8334545601315,2.1542844016961089,26.216084175503934,0.53141866308042374,2.5799446314641192E-2,0.50857405781631926,4.9632354813846863E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.0817971283657839,0.78119208241466886]
[21.8,2.5277426795420929E-2,39.833165708230432,1.2586360762770592,27.021350974091348,{"$f":"IF(ISERROR(F27),B27*Qone/(SQRT(I27)*$A27),(G27*Qone/SQRT(I27)*($A27+2*F27*root)^(2/3))^0.6/($A27+z*F27))","v":0.41741164362562999},{"$f":"($A27+2*F27*root)*(($A27+z*F27)*F27/($A27+2*F27*root))^(5/3)/(($A27*F27)^(5/3)/(B27*($A27+2*F27)^(2/3))+2*F27*(1+root)/ns*(z*F27/(2*(1+root)))^(5/3))","v":2.5770886348789317E-2},{"$f":"F27*($A27+z*F27)/($A27+2*F27*root)","v":0.40354903178817175},1.0357960427316357E-2,2.516278886860758E-2,23.671921741587823,2.1658301389791794,26.294355616593986,0.51876134966584575,2.5775766348752178E-2,0.49761344777397276,5.027494678830958E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.0861558838358214,0.78394858602982798]
[22.5,2.5284760765327485E-2,39.579210071878521,1.2607954908198602,27.068424810444935,{"$f":"IF(ISERROR(F28),B28*Qone/(SQRT(I28)*$A28),(G28*Qone/SQRT(I28)*($A28+2*F28*root)^(2/3))^0.6/($A28+z*F28))","v":0.40763176744112567},{"$f":"($A28+2*F28*root)*(($A28+z*F28)*F28/($A28+2*F28*root))^(5/3)/(($A28*F28)^(5/3)/(B28*($A28+2*F28)^(2/3))+2*F28*(1+root)/ns*(z*F28/(2*(1+root)))^(5/3))","v":2.5751413956261859E-2},{"$f":"F28*($A28+z*F28)/($A28+2*F28*root)","v":0.39478694037126133},1.0503854185041149E-2,2.5174934225472224E-2,23.518390818457355,2.1770812457364483,26.370596753505598,0.50676123124595784,2.5754792321442548E-2,0.48714203728229954,5.0923418362982644E-3,null,null,null,{"$f":"A28","v":22.5},{"$f":"QTone*2650*3600","v":38160},{"$f":"I28","v":1.0503854185041149E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.0904630165638314,0.78669773518369479]
[23.2,2.529192328089765E-2,39.336471166032993,1.2629032495699124,27.114464091419244,{"$f":"IF(ISERROR(F29),B29*Qone/(SQRT(I29)*$A29),(G29*Qone/SQRT(I29)*($A29+2*F29*root)^(2/3))^0.6/($A29+z*F29))","v":0.39835488965404947},{"$f":"($A29+2*F29*root)*(($A29+z*F29)*F29/($A29+2*F29*root))^(5/3)/(($A29*F29)^(5/3)/(B29*($A29+2*F29)^(2/3))+2*F29*(1+root)/ns*(z*F29/(2*(1+root)))^(5/3))","v":2.5733982058485486E-2},{"$f":"F29*($A29+z*F29)/($A29+2*F29*root)","v":0.38642780111006847},1.0649904986999054E-2,2.5186745995620763E-2,23.372245891240823,2.1880537251419439,26.444920447196964,0.49536663748644583,2.5736202418073815E-2,0.47712866786607827,5.1576816172753939E-3,null,null,null,{"$f":"A28","v":22.5},{"$f":"QTtwo*2650*3600","v":38160},{"$f":"Q28","v":5.0923418362982644E-3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.094718049188603,0.78943681613354777]
[23.9,2.5298923404672557E-2,39.10413589864568,1.2649620571664395,27.159522582965511,{"$f":"IF(ISERROR(F30),B30*Qone/(SQRT(I30)*$A30),(G30*Qone/SQRT(I30)*($A30+2*F30*root)^(2/3))^0.6/($A30+z*F30))","v":0.38954184439774542},{"$f":"($A30+2*F30*root)*(($A30+z*F30)*F30/($A30+2*F30*root))^(5/3)/(($A30*F30)^(5/3)/(B30*($A30+2*F30)^(2/3))+2*F30*(1+root)/ns*(z*F30/(2*(1+root)))^(5/3))","v":2.5718358289441922E-2},{"$f":"F30*($A30+z*F30)/($A30+2*F30*root)","v":0.37844460966883486},1.0796007200685846E-2,2.5198242853836789E-2,23.232935208971139,2.1987622720971784,26.517430170414837,0.48453125195453628,2.571972014898518E-2,0.46754458887098876,5.2234327925712821E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.0989208583420245,0.79216363167937487]
[24.6,2.5305769471590307E-2,38.881471879797942,1.2669744029395718,27.203649775350772,{"$f":"IF(ISERROR(F31),B31*Qone/(SQRT(I31)*$A31),(G31*Qone/SQRT(I31)*($A31+2*F31*root)^(2/3))^0.6/($A31+z*F31))","v":0.38115748718019604},{"$f":"($A31+2*F31*root)*(($A31+z*F31)*F31/($A31+2*F31*root))^(5/3)/(($A31*F31)^(5/3)/(B31*($A31+2*F31)^(2/3))+2*F31*(1+root)/ns*(z*F31/(2*(1+root)))^(5/3))","v":2.5704341973582682E-2},{"$f":"F31*($A31+z*F31)/($A31+2*F31*root)","v":0.37081263991794722},1.0942072164645676E-2,2.5209441930968426E-2,23.099962836870965,2.2092204143393506,26.588221036217579,0.47421343227475105,2.5705106933779451E-2,0.45836325995725419,5.289525913489173E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1030715971492311,0.79487640897998302]
[25.3,2.5312469166226297E-2,38.667817373955302,1.2689425836099661,27.246891334139406,{"$f":"IF(ISERROR(F32),B32*Qone/(SQRT(I32)*$A32),(G32*Qone/SQRT(I32)*($A32+2*F32*root)^(2/3))^0.6/($A32+z*F32))","v":0.3731701883270736},{"$f":"($A32+2*F32*root)*(($A32+z*F32)*F32/($A32+2*F32*root))^(5/3)/(($A32*F32)^(5/3)/(B32*($A32+2*F32)^(2/3))+2*F32*(1+root)/ns*(z*F32/(2*(1+root)))^(5/3))","v":2.569175908142033E-2},{"$f":"F32*($A32+z*F32)/($A32+2*F32*root)","v":0.3635092228214421},1.1088025378681783E-2,2.5220358980972246E-2,22.972881608860732,2.2194406348261291,26.657380688032475,0.4643756314688553,2.5692156062610862E-2,0.44956016675661692,5.3559014172506521E-3,null,"NOTE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.107170633887532,0.79757372501228851]
[26,2.5319029589944923E-2,38.462572742944452,1.2708687230402662,27.289289492550214,{"$f":"IF(ISERROR(F33),B33*Qone/(SQRT(I33)*$A33),(G33*Qone/SQRT(I33)*($A33+2*F33*root)^(2/3))^0.6/($A33+z*F33))","v":0.36555140132119918},{"$f":"($A33+2*F33*root)*(($A33+z*F33)*F33/($A33+2*F33*root))^(5/3)/(($A33*F33)^(5/3)/(B33*($A33+2*F33)^(2/3))+2*F33*(1+root)/ns*(z*F33/(2*(1+root)))^(5/3))","v":2.5680458098848717E-2},{"$f":"F33*($A33+z*F33)/($A33+2*F33*root)","v":0.3565135480078595},1.1233804207581095E-2,2.5231008525823814E-2,22.851287137259995,2.2294344783230535,26.724990073182038,0.45498390335057481,2.5680687749783427E-2,0.44111265016925383,5.4225080752265745E-3,null,"Cells for VBA output, STAB writes to these cells",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1112185032692299,0.80025444599226736]
[26.7,2.5325457319514067E-2,38.265193124817777,1.2727547894895963,27.330883394170819,{"$f":"IF(ISERROR(F34),B34*Qone/(SQRT(I34)*$A34),(G34*Qone/SQRT(I34)*($A34+2*F34*root)^(2/3))^0.6/($A34+z*F34))","v":0.3582752934222006},{"$f":"($A34+2*F34*root)*(($A34+z*F34)*F34/($A34+2*F34*root))^(5/3)/(($A34*F34)^(5/3)/(B34*($A34+2*F34)^(2/3))+2*F34*(1+root)/ns*(z*F34/(2*(1+root)))^(5/3))","v":2.5670306625564562E-2},{"$f":"F34*($A34+z*F34)/($A34+2*F34*root)","v":0.3498064858997727},1.1379355994559755E-2,2.5241403981738981E-2,22.734812697318791,2.2392126445969818,26.791124117843808,0.44600747807364577,2.567054505952E-2,0.43299974919526663,5.4893017148823055E-3,null,"Cells with formulas on these worksheet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1152158676396993,0.80291767791103685]
[27.4,2.533175845846097E-2,38.07518214278965,1.2746026107433341,27.371709393436308,{"$f":"IF(ISERROR(F35),B35*Qone/(SQRT(I35)*$A35),(G35*Qone/SQRT(I35)*($A35+2*F35*root)^(2/3))^0.6/($A35+z*F35))","v":0.35131842832011323},{"$f":"($A35+2*F35*root)*(($A35+z*F35)*F35/($A35+2*F35*root))^(5/3)/(($A35*F35)^(5/3)/(B35*($A35+2*F35)^(2/3))+2*F35*(1+root)/ns*(z*F35/(2*(1+root)))^(5/3))","v":2.566118855893797E-2},{"$f":"F35*($A35+z*F35)/($A35+2*F35*root)","v":0.34337042836126247},{"$f":"IF(ISERROR(I35),0.001,(G35/B35)^1.5*C35/(9810*H35))","v":1.152463650364027E-2},2.5251557769538566E-2,22.623124839560958,2.248785070200519,26.855852318243198,{"$f":"IF(ISERROR(N35),J35*Qtwo/(SQRT(Q35)*$A35),(O35*Qtwo/SQRT(Q35)*($A35+2*N35*root)^(2/3))^0.6/($A35+z*N35))","v":0.43741839649350678},{"$f":"($A35+2*N35*root)*(($A35+z*N35)*N35/($A35+2*N35*root))^(5/3)/(($A35*N35)^(5/3)/(J35*($A35+2*N35)^(2/3))+2*N35*(1+root)/ns*(z*N35/(2*(1+root)))^(5/3))","v":2.5661590532454016E-2},{"$f":"N35*($A35+z*N35)/($A35+2*N35*root)","v":0.42520205682990503},{"$f":"IF(ISERROR(Q35),0.001,(O35/J35)^1.5*K35/(9810*P35))","v":5.5562441616622263E-3},null,"Two things consntrain moving cells on this worksheet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Qone/(A35*SQRT(9.81)*F35^1.5)","v":1.1191634860016877},{"$f":"Qtwo/(A35*SQRT(9.81)*N35^1.5)","v":0.80556272597012191}]
[28.1,2.5337938682229298E-2,37.89208647702236,1.2764138874268833,27.411801320015574,{"$f":"IF(ISERROR(F36),B36*Qone/(SQRT(I36)*$A36),(G36*Qone/SQRT(I36)*($A36+2*F36*root)^(2/3))^0.6/($A36+z*F36))","v":0.34465949245806232},{"$f":"($A36+2*F36*root)*(($A36+z*F36)*F36/($A36+2*F36*root))^(5/3)/(($A36*F36)^(5/3)/(B36*($A36+2*F36)^(2/3))+2*F36*(1+root)/ns*(z*F36/(2*(1+root)))^(5/3))","v":2.5653001750787732E-2},{"$f":"F36*($A36+z*F36)/($A36+2*F36*root)","v":0.33718914595257915},1.1669608627638356E-2,2.5261481411498917E-2,22.515919610701925,2.2581610004956754,26.919239260336607,0.42919119404716344,2.565370337840794E-2,0.41770158833430926,5.6233023586633006E-3,null,"First, the STAB VBA code writes to certain cells. You can't change these locations without changing the VBA code.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.123062189244999,0.8081890611797824]
[28.8,2.5344003278019892E-2,37.715491162626343,1.2781902047607785,27.451190712223738,{"$f":"IF(ISERROR(F37),B37*Qone/(SQRT(I37)*$A37),(G37*Qone/SQRT(I37)*($A37+2*F37*root)^(2/3))^0.6/($A37+z*F37))","v":0.33827905816116238},{"$f":"($A37+2*F37*root)*(($A37+z*F37)*F37/($A37+2*F37*root))^(5/3)/(($A37*F37)^(5/3)/(B37*($A37+2*F37)^(2/3))+2*F37*(1+root)/ns*(z*F37/(2*(1+root)))^(5/3))","v":2.5645656048310716E-2},{"$f":"F37*($A37+z*F37)/($A37+2*F37*root)","v":0.33124766003335476},1.181424131180242E-2,2.5271185616635231E-2,22.412919285880971,2.2673490532920049,26.981345078188912,0.42130262649564154,2.5646777129364969E-2,0.41048166107665074,5.6904476308377938E-3,null,"Second, charts on the worksheet STAB OUTPUT reference particular cells on this worksheet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1269128603167802,0.81079629275185339]
[29.5,2.5349957180054228E-2,37.545015501632825,1.279933042972786,27.489907023750451,{"$f":"IF(ISERROR(F38),B38*Qone/(SQRT(I38)*$A38),(G38*Qone/SQRT(I38)*($A38+2*F38*root)^(2/3))^0.6/($A38+z*F38))","v":0.33215937791434347},{"$f":"($A38+2*F38*root)*(($A38+z*F38)*F38/($A38+2*F38*root))^(5/3)/(($A38*F38)^(5/3)/(B38*($A38+2*F38)^(2/3))+2*F38*(1+root)/ns*(z*F38/(2*(1+root)))^(5/3))","v":2.5639071648744776E-2},{"$f":"F38*($A38+z*F38)/($A38+2*F38*root)","v":0.3255321281149029},1.1958508653449641E-2,2.5280680356044128E-2,22.313869532447622,2.2763572752526673,27.042225859582206,0.41373143119559286,2.5640717668395614E-2,0.40352678508887935,5.7576550673151781E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.130716418340286,0.81338414520222546]
[30.2,2.5355805000881394E-2,37.3803094962663,1.2816437865482708,27.527977807308577,{"$f":"IF(ISERROR(F39),B39*Qone/(SQRT(I39)*$A39),(G39*Qone/SQRT(I39)*($A39+2*F39*root)^(2/3))^0.6/($A39+z*F39))","v":0.32628420510445583},{"$f":"($A39+2*F39*root)*(($A39+z*F39)*F39/($A39+2*F39*root))^(5/3)/(($A39*F39)^(5/3)/(B39*($A39+2*F39)^(2/3))+2*F39*(1+root)/ns*(z*F39/(2*(1+root)))^(5/3))","v":2.5633177711557008E-2},{"$f":"F39*($A39+z*F39)/($A39+2*F39*root)","v":0.32002974101914872},1.2102389145934532E-2,2.5289975729930716E-2,22.218537027898172,2.2851936913030011,27.101939151612907,0.40645812891274169,2.5635442386054863E-2,0.39682257327552145,5.824902882692367E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1344738059000261,0.81595240835837057]
[30.9,2.5361551059253376E-2,37.221050726632384,1.2833237324722107,27.565428878252906,{"$f":"IF(ISERROR(F40),B40*Qone/(SQRT(I40)*$A40),(G40*Qone/SQRT(I40)*($A40+2*F40*root)^(2/3))^0.6/($A40+z*F40))","v":0.32063863733061232},{"$f":"($A40+2*F40*root)*(($A40+z*F40)*F40/($A40+2*F40*root))^(5/3)/(($A40*F40)^(5/3)/(B40*($A40+2*F40)^(2/3))+2*F40*(1+root)/ns*(z*F40/(2*(1+root)))^(5/3))","v":2.56279111830441E-2},{"$f":"F40*($A40+z*F40)/($A40+2*F40*root)","v":0.31472863055117456},1.2245865041527866E-2,2.5299078025646654E-2,22.126706859107973,2.2938638530200968,27.160518553253073,0.39946478986257788,2.5630874678687438E-2,0.3903556018603464,5.8921725667219109E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1381859788738216,0.81850107615794132]
[31.6,2.5367199405013294E-2,37.066941608741772,1.2849740975928954,27.602284460754074,{"$f":"IF(ISERROR(F41),B41*Qone/(SQRT(I41)*$A41),(G41*Qone/SQRT(I41)*($A41+2*F41*root)^(2/3))^0.6/($A41+z*F41))","v":0.31520897902911532},{"$f":"($A41+2*F41*root)*(($A41+z*F41)*F41/($A41+2*F41*root))^(5/3)/(($A41*F41)^(5/3)/(B41*($A41+2*F41)^(2/3))+2*F41*(1+root)/ns*(z*F41/(2*(1+root)))^(5/3))","v":2.5623215796941507E-2},{"$f":"F41*($A41+z*F41)/($A41+2*F41*root)","v":0.30961778653131566},1.2388921812688402E-2,2.5307997773184536E-2,22.038181512735829,2.3023758712308431,27.218025457250061,0.39273497607386959,2.562695093964262E-2,0.38411342600371506,5.9594473295784128E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1418538983191029,0.82103002394420777]
[32.299999999999997,2.5372753841375249E-2,36.917706979230466,1.2865960252181272,27.638567318730185,{"$f":"IF(ISERROR(F42),B42*Qone/(SQRT(I42)*$A42),(G42*Qone/SQRT(I42)*($A42+2*F42*root)^(2/3))^0.6/($A42+z*F42))","v":0.3099826206850011},{"$f":"($A42+2*F42*root)*(($A42+z*F42)*F42/($A42+2*F42*root))^(5/3)/(($A42*F42)^(5/3)/(B42*($A42+2*F42)^(2/3))+2*F42*(1+root)/ns*(z*F42/(2*(1+root)))^(5/3))","v":2.5619041221517938E-2},{"$f":"F42*($A42+z*F42)/($A42+2*F42*root)","v":0.3046869821599229},1.2531547695085585E-2,2.5316741789836589E-2,21.952778326939221,2.3107354591976113,27.274497850331333,0.38625349736149711,2.5623611350324847E-2,0.37808440695924461,6.0267129634786285E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1454785240199417,0.82353930670138287]
[33,2.5378217944919283E-2,36.773091961687889,1.2881905910386815,27.674298873419303,{"$f":"IF(ISERROR(F43),B43*Qone/(SQRT(I43)*$A43),(G43*Qone/SQRT(I43)*($A43+2*F43*root)^(2/3))^0.6/($A43+z*F43))","v":0.30494793233426176},{"$f":"($A43+2*F43*root)*(($A43+z*F43)*F43/($A43+2*F43*root))^(5/3)/(($A43*F43)^(5/3)/(B43*($A43+2*F43)^(2/3))+2*F43*(1+root)/ns*(z*F43/(2*(1+root)))^(5/3))","v":2.5615342329094948E-2},{"$f":"F43*($A43+z*F43)/($A43+2*F43*root)","v":0.29992670680300421},1.2673733298811555E-2,2.5325317223842906E-2,21.870328464598703,2.3189484611166717,27.329976270847713,0.38000633792094318,2.5620803099924542E-2,0.37225769296024397,6.0939569797050838E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1490608093793813,0.82602899496924065]
[33.700000000000003,2.5383595083578982E-2,36.632860076541746,1.2897588084603093,27.709499309208564,{"$f":"IF(ISERROR(F44),B44*Qone/(SQRT(I44)*$A44),(G44*Qone/SQRT(I44)*($A44+2*F44*root)^(2/3))^0.6/($A44+z*F44))","v":0.30009416941736017},{"$f":"($A44+2*F44*root)*(($A44+z*F44)*F44/($A44+2*F44*root))^(5/3)/(($A44*F44)^(5/3)/(B44*($A44+2*F44)^(2/3))+2*F44*(1+root)/ns*(z*F44/(2*(1+root)))^(5/3))","v":2.5612078568293291E-2},{"$f":"F44*($A44+z*F44)/($A44+2*F44*root)","v":0.29532810539028631},1.2815471276681239E-2,2.5333730792161814E-2,21.790675526072338,2.3270203818371864,27.38449886981277,0.37398053556189442,2.5618478815592174E-2,0.36662314746810226,6.1611684927379258E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1526016974032798,0.82849919787460635]
[34.4,2.5388888432860305E-2,36.496791562266502,1.2913016334143421,27.744187669110669,{"$f":"IF(ISERROR(F45),B45*Qone/(SQRT(I45)*$A45),(G45*Qone/SQRT(I45)*($A45+2*F45*root)^(2/3))^0.6/($A45+z*F45))","v":0.29541138934007127},{"$f":"($A45+2*F45*root)*(($A45+z*F45)*F45/($A45+2*F45*root))^(5/3)/(($A45*F45)^(5/3)/(B45*($A45+2*F45)^(2/3))+2*F45*(1+root)/ns*(z*F45/(2*(1+root)))^(5/3))","v":2.5609213422806427E-2},{"$f":"F45*($A45+z*F45)/($A45+2*F45*root)","v":0.29088292370944896},1.2956756040494812E-2,2.5341988814705424E-2,21.713674397218902,2.3349564130208758,27.438101597171052,0.36816408362773861,2.5616595915163614E-2,0.36117129277651777,6.228338019004959E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1561021175709276,0.83095005645611575]
[35.1,2.5394100990497884E-2,36.364681880509671,1.2928199687073032,27.778381941089371,{"$f":"IF(ISERROR(F46),B46*Qone/(SQRT(I46)*$A46),(G46*Qone/SQRT(I46)*($A46+2*F46*root)^(2/3))^0.6/($A46+z*F46))","v":0.29089037734343448},{"$f":"($A46+2*F46*root)*(($A46+z*F46)*F46/($A46+2*F46*root))^(5/3)/(($A46*F46)^(5/3)/(B46*($A46+2*F46)^(2/3))+2*F46*(1+root)/ns*(z*F46/(2*(1+root)))^(5/3))","v":2.5606713943323971E-2},{"$f":"F46*($A46+z*F46)/($A46+2*F46*root)","v":0.28658345896225884},1.309758351772951E-2,2.5350097245227191E-2,21.639190225110202,2.3427614568048143,27.49081837008708,0.36254584372553572,2.5615116047595966E-2,0.35589325864450405,6.2954573032509443E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1595629834265961,0.83338173802083026]
[35.799999999999997,2.5399235589727162E-2,36.236340381756307,1.2943146679620037,27.812099136274799,{"$f":"IF(ISERROR(F47),B47*Qone/(SQRT(I47)*$A47),(G47*Qone/SQRT(I47)*($A47+2*F47*root)^(2/3))^0.6/($A47+z*F47))","v":0.28652258048973905},{"$f":"($A47+2*F47*root)*(($A47+z*F47)*F47/($A47+2*F47*root))^(5/3)/(($A47*F47)^(5/3)/(B47*($A47+2*F47)^(2/3))+2*F47*(1+root)/ns*(z*F47/(2*(1+root)))^(5/3))","v":2.5604550341512339E-2},{"$f":"F47*($A47+z*F47)/($A47+2*F47*root)","v":0.28242251502093935},1.3237950942419714E-2,2.535806169924839E-2,21.567097505043325,2.3504401472499294,27.542681225311249,0.35711546789778281,2.5614004607805278E-2,0.3507807354771515,6.3625191683338534E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1629851907574897,0.83579443136673925]
[36.5,2.5404294911327459E-2,36.111589111517283,1.2957865391956027,27.845355359973347,{"$f":"IF(ISERROR(F48),B48*Qone/(SQRT(I48)*$A48),(G48*Qone/SQRT(I48)*($A48+2*F48*root)^(2/3))^0.6/($A48+z*F48))","v":0.28230004874334486},{"$f":"($A48+2*F48*root)*(($A48+z*F48)*F48/($A48+2*F48*root))^(5/3)/(($A48*F48)^(5/3)/(B48*($A48+2*F48)^(2/3))+2*F48*(1+root)/ns*(z*F48/(2*(1+root)))^(5/3))","v":2.5602695636819054E-2},{"$f":"F48*($A48+z*F48)/($A48+2*F48*root)","v":0.27839336188731739},1.3377856675033946E-2,2.5365887479359146E-2,21.497279264843179,2.3579968698209677,27.593720457409432,0.35186332906205414,2.5613230314825781E-2,0.34582593161900654,6.4295173849553099E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1663696162486006,0.83818834273371468]
[37.200000000000003,2.5409281494570998E-2,35.990261739856336,1.2972363480744062,27.878165876260695,{"$f":"IF(ISERROR(F49),B49*Qone/(SQRT(I49)*$A49),(G49*Qone/SQRT(I49)*($A49+2*F49*root)^(2/3))^0.6/($A49+z*F49))","v":0.27821538226964282},{"$f":"($A49+2*F49*root)*(($A49+z*F49)*F49/($A49+2*F49*root))^(5/3)/(($A49*F49)^(5/3)/(B49*($A49+2*F49)^(2/3))+2*F49*(1+root)/ns*(z*F49/(2*(1+root)))^(5/3))","v":2.5601125348386818E-2},{"$f":"F49*($A49+z*F49)/($A49+2*F49*root)","v":0.27448969891397701},1.3517300047017285E-2,2.5373579598185751E-2,21.429626334441032,2.3654357791122331,27.64396474441018,0.34678045870869256,2.5612764844033738E-2,0.34102153436715638,6.4964465584057985E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1697171165251512,0.84056369236883344]
[37.9,2.5414197747195815E-2,35.872202599451299,1.2986648208800065,27.910545166846649,{"$f":"IF(ISERROR(F50),B50*Qone/(SQRT(I50)*$A50),(G50*Qone/SQRT(I50)*($A50+2*F50*root)^(2/3))^0.6/($A50+z*F50))","v":0.27426168419733171},{"$f":"($A50+2*F50*root)*(($A50+z*F50)*F50/($A50+2*F50*root))^(5/3)/(($A50*F50)^(5/3)/(B50*($A50+2*F50)^(2/3))+2*F50*(1+root)/ns*(z*F50/(2*(1+root)))^(5/3))","v":2.5599817225608473E-2},{"$f":"F50*($A50+z*F50)/($A50+2*F50*root)","v":0.27070562139663745},1.3656281226370597E-2,2.5381142799278996E-2,21.364036690394091,2.3727608150065476,27.693441262229062,0.34185849098548088,2.5612582505672644E-2,0.33636067434971356,6.5633020298746896E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1730285275096433,0.84292071161098059]
[38.6,2.5419045954505913E-2,35.757265819402775,1.3000726472172852,27.942506984815818,{"$f":"IF(ISERROR(F51),B51*Qone/(SQRT(I51)*$A51),(G51*Qone/SQRT(I51)*($A51+2*F51*root)^(2/3))^0.6/($A51+z*F51))","v":0.27043251819231212},{"$f":"($A51+2*F51*root)*(($A51+z*F51)*F51/($A51+2*F51*root))^(5/3)/(($A51*F51)^(5/3)/(B51*($A51+2*F51)^(2/3))+2*F51*(1+root)/ns*(z*F51/(2*(1+root)))^(5/3))","v":2.559875101188025E-2},{"$f":"F51*($A51+z*F51)/($A51+2*F51*root)","v":0.26703559019104639},1.3794801101219464E-2,2.5388581281507266E-2,21.300414831162577,2.3799755348569875,27.742173857342571,0.33708960931305609,2.5612659664124047E-2,0.33183688994321558,6.63007983867747E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1763046640337824,0.84525965208584042]
[39.299999999999997,2.5423828287689364E-2,35.645314543709752,1.3014604824908746,27.974064403774513,{"$f":"IF(ISERROR(F52),B52*Qone/(SQRT(I52)*$A52),(G52*Qone/SQRT(I52)*($A52+2*F52*root)^(2/3))^0.6/($A52+z*F52))","v":0.26672187027902983},{"$f":"($A52+2*F52*root)*(($A52+z*F52)*F52/($A52+2*F52*root))^(5/3)/(($A52*F52)^(5/3)/(B52*($A52+2*F52)^(2/3))+2*F52*(1+root)/ns*(z*F52/(2*(1+root)))^(5/3))","v":2.5597908236959621E-2},{"$f":"F52*($A52+z*F52)/($A52+2*F52*root)","v":0.26347440404653089},1.3932861178804132E-2,2.5395899831659161E-2,21.238671379200902,2.3870838181820511,27.790190450505857,0.33246651288256202,2.5612975622465214E-2,0.32744410888855774,6.69677646405105E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1795463196562741,0.84758073945651013]
[40,2.5428546811434177E-2,35.536220224789261,1.3028289501736994,28.005229862870735,{"$f":"IF(ISERROR(F53),B53*Qone/(SQRT(I53)*$A53),(G53*Qone/SQRT(I53)*($A53+2*F53*root)^(2/3))^0.6/($A53+z*F53))","v":0.26312411441960309},{"$f":"($A53+2*F53*root)*(($A53+z*F53)*F53/($A53+2*F53*root))^(5/3)/(($A53*F53)^(5/3)/(B53*($A53+2*F53)^(2/3))+2*F53*(1+root)/ns*(z*F53/(2*(1+root)))^(5/3))","v":2.5597272034036722E-2},{"$f":"F53*($A53+z*F53)/($A53+2*F53*root)","v":0.2600171743825907},1.407046349772006E-2,2.5403102254661202E-2,21.178722412289464,2.3940888961149547,27.837512736996018,0.32798235892276828,2.5613510794889389E-2,0.32317660465888454,6.763389018334673E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.182754266646264,0.84988423437683258]
[null,"Case 1 Surface",null,null,null,null,null,null,null,"Case 2 Surface"]
[null,"GSD @ mean width",null,null,"For convenient local reference",null,null,null,null,"GSD @ mean width"]
[null,"D (mm)","Fi (%ft)",{"$f":"Qone","v":20},null,null,null,null,null,"D (mm)","Fi (%ft)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Qone","v":20},{"$f":"Qtwo","v":20}]
[null,64,100,{"$f":"Qtwo","v":20},null,null,null,null,null,64,100]
[null,45.25,82.709989839311405,{"$f":"QTone*2650*3600","v":38160},null,null,null,null,null,45.25,79.922804545478215]
[null,32,61.807435796295877,{"$f":"QTtwo*2650*3600","v":38160},null,null,null,null,null,32,60.707293311400484]
[null,22.63,37.365500260749613,null,null,null,null,null,null,22.63,41.534652136051896]
[null,16,17.433995539361206,null,null,null,null,null,null,16,26.961728941692375]
[null,11.31,8.7318712937580223,null,null,null,null,null,null,11.31,20.728313391709293]
[null,8,4.8093212702298702,null,null,null,null,null,null,8,17.909780840225558]
[null,5.66,1.9369256434412185,null,null,null,null,null,null,5.66,15.81697405504574]
[null,4,0.61274483262311019,null,null,null,null,null,null,4,14.833895240215497]
[null,2.83,0,null,null,null,null,null,null,2.83,14.099586076597635]
[null,null,null,null,null,null,null,null,null,2,13.58821281529433]
[null,null,null,null,null,null,null,null,null,1.4,12.618416902862229]
[null,null,null,null,null,null,null,null,null,1,11.006475676392066]
[null,null,null,null,null,null,null,null,null,0.70699999999999996,7.9401904270409362]
[null,null,null,null,null,null,null,null,null,0.5,4.607398519889415]
[null,null,null,null,null,null,null,null,null,0.35,2.2300558046651839]
[null,null,null,null,null,null,null,null,null,0.25,0.72031375311026657]
[null,null,null,null,null,null,null,null,null,0.17699999999999999,0]

{"sheet":"STATE","index":6,"n_rows":57,"n_cols":11,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
["STATE DIAGRAM FOR GRAVEL-BED RIVERS WORKSHEET"]
[]
["RULES, CONVENTIONS, AND UNITS"]
["1. Cells for input data are highlighted in GREEN"]
["2. LIGHT GREEN cells can be changed, but their default values are recommended"]
["3. Grain-diameters must be in millimeters (mm)"]
["4. Cumulative percentiles, not fractions, are used"]
["5. Cumulative grain-size distribution percentiles must span from 0 to 100 %"]
["6.  The 0 and 100 % must be EXACTLY 0 and 100"]
["INSTRUCTIONS"]
["1. In table below, enter grain size and cumulative % in order of decreasing grain size"]
["2. Check input for errors, press Enter, and then click once on the Run STATE button"]
["3. Plots will appear in the separate worksheets \"STATE I OUTPUT\" and \"STATE II OUTPUT\""]
[]
["D (mm)","FIRST Transport CDF GSD (% Finer)","SECOND Transport CDF GSD (% Finer)",null,"qT (m2/s)","S (%/100)",null,"Statistic","FIRST Transport GSD","SECOND Transport GSD","Units"]
[64,100,100,null,5.0000000000000001E-9,1E-4,null,"Dmin",0.17699999999999999,0.17699999999999999,"mm"]
[45.25,93.670886075949369,95.780590717299575,null,1E-8,2.0000000000000001E-4,null,"Dmax",64,64,"mm"]
[32,78.481012658227854,85.654008438818565,null,2E-8,5.0000000000000001E-4,null,"D50",21.670253040365619,14.798649106475827,"mm"]
[22.63,53.164556962025323,68.776371308016877,null,4.9999999999999998E-8,1E-3,null,"Dg",20.232789530422835,7.4694186121726753,"mm"]
[16,27.848101265822791,51.898734177215189,null,9.9999999999999995E-8,2E-3,null,"sg",0.85959126638007455,1.3700131291900819,"f/y-units"]
[11.31,15.189873417721525,43.459915611814345,null,1.9999999999999999E-7,5.0000000000000001E-3,null,"Fs",0,0,"%"]
[8,8.8607594936708924,39.240506329113927,null,4.9999999999999998E-7,0.01]
[5.66,3.7974683544303858,35.864978902953588,null,9.9999999999999995E-7,0.02]
[4,1.2658227848101324,34.177215189873422,null,1.9999999999999999E-6,0.05]
[2.83,0,32.843137254901961,null,5.0000000000000004E-6,0.1]
[2,null,31.862745098039216,null,1.0000000000000001E-5]
[1.4,null,29.901960784313729,null,2.0000000000000002E-5]
[1,null,26.47058823529412,null,5.0000000000000002E-5]
[0.70699999999999996,null,19.607843137254903,null,1E-4]
[0.5,null,11.764705882352942,null,2.0000000000000001E-4]
[0.35,null,5.8823529411764701,null,5.0000000000000001E-4]
[0.25,null,1.960784313725489,null,1E-3]
[0.17699999999999999,null,0,null,2E-3]
[null,null,null,null,5.0000000000000001E-3]
[null,null,null,null,0.01]
[null,null,null,null,0.02]
[null,null,null,null,0.05]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["PLOT DATA"]
["D (mm)","GSD 1 Mean & STD"]
[{"$f":"2^((LOG(I19)/LOG(2))-I20)","v":11.150465765513838},16]
[{"$f":"I19","v":20.232789530422835},50]
[{"$f":"2^((LOG(I19)/LOG(2))+I20)","v":36.712885433761365},84]
["D (mm)","GSD 2 Mean & STD"]
[{"$f":"2^((LOG(J19)/LOG(2))-J20)","v":2.8898263927057988},16]
[{"$f":"J19","v":7.4694186121726753},50]
[{"$f":"2^((LOG(J19)/LOG(2))+J20)","v":19.306424269878811},84]

{"sheet":"STATE I OUTPUT","index":7,"n_rows":34,"n_cols":16,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["State diagram developed using inverse calculation of the Wilcock & Crowe (2003) transport relation.  "]
["1. DIMENSIONLESS STATE DIAGRAM"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["2. DIMENSIONED STATE DIAGRAM",null,null,null,"òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò"]

{"sheet":"STATE II OUTPUT","index":8,"n_rows":34,"n_cols":18,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["State diagram developed using inverse calculation of the Wilcock & Crowe (2003) transport relation.  "]
["1. DIMENSIONLESS SLOPE/TRANSPORT STATE DIAGRAM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3. Tramsport rate for q*t = 0.01 and 0.1"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["2. DIMENSIONED SLOPE/TRANSPORT STATE DIAGRAM",null,null,null,null,null,"òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò","òòòòò"]

{"sheet":"STATE plot DATA","index":9,"n_rows":211,"n_cols":35,"rows_kept":211,"cut":false,"hidden":true,"merged":[]}
["DIMENSIONLESS STANDARD STATE DIAGRAM FIRST GSD RESULTS",null,null,null,null,null,null,null,null,null,null,null,"GAMMAS"]
["S=0.0001","S=0.0002","S=0.0005","S=0.001","S=0.002","S=0.005","S=0.01","S=0.02","S=0.05","S=0.1","q*T",null,"q*W","G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.12","G1=1.58,G2=4.12","G1=1.58,G2=4.11","G1=1.58,G2=4.09","G1=1.55,G2=4.02","G1=1.51,G2=3.93","G1=1.45,G2=3.76","G1=1.36,G2=3.41","G1=1.3,G2=3.07","G1=1.25,G2=2.74","G1=1.2,G2=2.35","G1=1.16,G2=2.1","G1=1.13,G2=1.88","G1=1.1,G2=1.63","G1=1.08,G2=1.49","G1=1.07,G2=1.36","G1=1.05,G2=1.23"]
[2013.9221994271461,897.10035295200851,308.01912590772059,137.20692221694802,61.118735561530116,20.985098759909562,9.3477987926259267,4.1639709808921248,1.4296981353524441,0.63685811805656312,4.3182708913419167E-7,null,0.63685811805656312,4.3182708913419167E-7,8.6365417826838334E-7,1.7273083565367667E-6,4.3182708913419169E-6,8.6365417826838338E-6,1.7273083565367668E-5,4.3182708913419166E-5,8.6365417826838331E-5,1.7273083565367666E-4,4.318270891341917E-4,8.6365417826838339E-4,1.7273083565367668E-3,4.3182708913419169E-3,8.6365417826838337E-3,1.7273083565367667E-2,4.3182708913419167E-2,8.6365417826838334E-2,0.17273083565367667,0.43182708913419171,0.86365417826838342,1.7273083565367668,4.3182708913419168]
[2289.7548345020914,1019.9698234567788,350.20632021779619,155.99918088333993,69.489735139955215,23.859278849835729,10.628100471535779,4.7342805431789809,1.6255137453835435,0.72408405604085069,8.6365417826838334E-7,null,445725.45176967635,4.3182708913419167E-7,8.6365417826838334E-7,1.7273083565367667E-6,4.3182708913419169E-6,8.6365417826838338E-6,1.7273083565367668E-5,4.3182708913419166E-5,8.6365417826838331E-5,1.7273083565367666E-4,4.318270891341917E-4,8.6365417826838339E-4,1.7273083565367668E-3,4.3182708913419169E-3,8.6365417826838337E-3,1.7273083565367667E-2,4.3182708913419167E-2,8.6365417826838334E-2,0.17273083565367667,0.43182708913419171,0.86365417826838342,1.7273083565367668,4.3182708913419168]
[2603.366308597745,1159.6678535897388,398.17159521851477,177.36528189003442,79.007251139215796,27.127114994653091,12.08375598779101,5.3827013599218292,1.8481488302280449,0.82325671189136684,1.7273083565367667E-6]
[3084.806123610449,1374.1249106180089,471.80535874700121,210.16539465972318,93.618040349902927,32.143724905337812,14.318401657210579,6.378122841113707,2.1899264847987516,0.97550134906439401,4.3182708913419169E-6]
[3507.3101319643119,1562.3290503438147,536.42519132180621,238.95025766339171,106.44023912580971,36.546222849044604,16.279491544542509,7.2516890745047062,2.4898651781078933,1.1091088477592956,8.6365417826838338E-6]
[3987.6815167178815,1776.3101757979423,609.89554389300463,271.67757912689143,121.01860349580907,41.551699700809571,18.509178000001786,8.2449014770164784,2.8308843462039621,1.2610156176183316,1.7273083565367668E-5]
[4725.0405180195821,2104.7662703324049,722.67084133286767,321.91326309042614,143.39605671981721,49.234991273952694,21.931695306807626,9.7694596177397042,3.3543409075081896,1.4941890073523747,4.3182708913419166E-5]
[5369.8598360897868,2392.0006222828415,821.29266633528971,365.84429182808555,162.96510531430079,55.954017994969931,24.924681453260096,11.102683378382853,3.8121028691899457,1.698098779790217,8.6365417826838331E-5]
[6091.4631404642432,2713.4383517193596,931.65821031150006,415.00655265571902,184.86440289041064,63.473134975795901,28.274067293142654,12.594665154037241,4.3243743457255235,1.9262897806829193,1.7273083565367666E-4]
[7154.8707566011244,3187.13259275787,1094.3009799772128,487.455670160708,217.13681584820736,74.55385788208298,33.209968209782382,14.79335905378827,5.0792952092737504,2.2625687954991767,4.318270891341917E-4]
[8074.2906974124617,3596.6876161086138,1234.9215692886528,550.09502154155848,245.03947477337834,84.13422710649705,37.477537540453213,16.694345076923103,5.7319981663977781,2.5533149094132788,8.6365417826838339E-4]
[9182.0018794154876,4090.1168521667219,1404.3403433285994,625.5625058521066,278.6564172901501,95.676593816790898,42.619077393706469,18.984640709188501,6.518370456185961,2.9036039418899673,1.7273083565367668E-3]
[11196.442395930431,4987.4480891332842,1712.4387431905827,762.80474060117194,339.79088279647902,116.66709344833266,51.969282001139383,23.14968335874444,7.9484365486393074,3.5406259662012922,4.3182708913419169E-3]
[13527.820666114747,6025.9590453370083,2069.0111555442927,921.63969314623625,410.54381060561872,140.96008910647743,62.790581346954376,27.970024216644173,9.603499076194657,4.2778725083218783,8.6365417826838337E-3]
[16966.294699897462,7557.6250998649393,2594.9082168326622,1155.9002020340261,514.89500414513645,176.78903880614288,78.750564026827703,35.079388272164756,12.044497003500528,5.3652134705318915,1.7273083565367667E-2]
[24330.627131710695,10838.062261595809,3721.2452914158894,1657.6263300040948,738.38858627816148,253.5254904060927,112.93276720934445,50.305828771423151,17.272490591770119,7.6940198636495358,4.3182708913419167E-2]
[33538.393385452597,14939.655837793074,5129.5261643547383,2284.9441422454838,1017.8269036743892,349.47054938001867,155.67143223522942,69.343739714718282,23.809151366193532,10.605771216075565,8.6365417826838334E-2]
[48235.275160834084,21486.372404966813,7377.3392523229741,3286.2310415904735,1463.8495112329722,502.61227233576312,223.88831457276726,99.730906229739688,34.242575495355553,15.253333307318035,0.17273083565367667]
[83221.26083906347,37070.85730177223,12728.267272627605,5669.798498665783,2525.6081072876832,867.16675456911935,386.27887502977336,172.06767730435868,59.079383243867255,26.316873400241601,0.43182708913419171]
[131909.78758112006,58759.130333092151,20174.929041929718,8986.9092110137444,4003.2129480678759,1374.5019150073847,612.27099708076037,272.73572322687841,93.643725359951105,41.713537442533216,0.86365417826838342]
[217502.75925459142,96886.464705951148,33265.937386843027,14818.290487837619,6600.7980003228586,2266.3819311434868,1009.5583786360797,449.70713270736132,154.4068035144324,68.780411661577546,1.7273083565367668]
[445725.45176967635,198548.11681206414,68171.433875634248,30366.92152679573,13526.925731045294,4644.4657235778841,2068.8742797911405,921.57872192972229,316.42376624851579,140.95076386997056,4.3182708913419168]
[]
["DIMENSIONLESS STANDARD STATE DIAGRAM SECOND GSD RESULTS"]
["S=0.0001","S=0.0002","S=0.0005","S=0.001","S=0.002","S=0.005","S=0.01","S=0.02","S=0.05","S=0.1","q*T"]
[5253.34743617601,2340.1002484175224,803.47268918370935,357.90639442726894,159.42917400474226,54.739957084553346,24.383878798842883,10.861783182589258,3.7293898622279351,1.6612543238522228,4.3182708913419167E-7]
[5972.8611625239446,2660.6071766613991,913.51864286123362,406.92629396118775,181.26505683381049,62.237300631795051,27.723565676690573,12.349444561821569,4.2401779320018012,1.8887845421536804,8.6365417826838334E-7]
[6790.9215790903772,3025.0116649015927,1038.6368100487114,462.66010134288405,206.09164561052739,70.761502131784709,31.520665771445948,14.040860365355631,4.8209250197012938,2.1474779601512872,1.7273083565367667E-6]
[8046.7648378763888,3584.4262396204149,1230.7116295022142,548.21970656196549,244.20411691766398,83.847407247725855,37.349773818194983,16.637432808730757,5.7124573568948636,2.5446104683444939,4.3182708913419169E-6]
[9148.8731267125895,4075.3596705084215,1399.2734696167636,623.30547020467986,277.65102220760531,95.331391729311704,42.465307345089172,18.916143939587737,6.4948521117437776,2.8931277104318047,8.6365417826838338E-6]
[10399.839899360668,4632.6020176025868,1590.6024553940031,708.53284429069686,315.61550136945516,108.36648378840538,48.271780748233112,21.502633795476193,7.3829225956738709,3.2887181383076003,1.7273083565367668E-5]
[12276.721804465271,5468.6578592818305,1877.6619674281721,836.40331994131304,372.5753227920199,127.92362067805816,56.983494840976512,25.383261254491302,8.7153348213140021,3.8822403102362562,4.3182708913419166E-5]
[13786.800296735693,6141.3213558093385,2108.6207688026689,939.2837699851973,418.40335332491873,143.65866064361592,63.992658308577717,28.50548862875231,9.7873506147984592,4.3597690583570063,8.6365417826838331E-5]
[15262.877296355222,6798.8389092280768,2334.3792153427712,1039.8477253011631,463.19950276597683,159.03940455867766,70.844000827564386,31.55741476260512,10.835228499352764,4.8265455904155283,1.7273083565367666E-4]
[16972.918886942134,7560.5758397383497,2595.9213524463066,1156.3515026437753,515.09603571249727,176.85806293198851,78.781310779446017,35.093084393412077,12.049199562451756,5.3673082224027064,4.318270891341917E-4]
[17873.711441558615,7961.8333058474427,2733.6929780712067,1217.7217849764422,542.43338864353916,186.24433451993519,82.962419442355412,36.955556567507799,12.688678801540972,5.6521638395936771,8.6365417826838339E-4]
[18329.131522524774,8164.6998890215027,2803.3471560230269,1248.7491939016402,556.2545280628766,190.9898184214679,85.076292204770965,37.897179834681694,13.011984856136618,5.7961803143968131,1.7273083565367668E-3]
[18709.408434983743,8334.0939959455336,2861.508569712104,1274.6571583520547,567.79521422212645,194.95230940862464,86.841381275321254,38.683437629860087,13.281946224462972,5.9164344328914931,4.3182708913419169E-3]
[19422.04999469527,8651.5397219657989,2970.5034605625538,1323.2088626233106,589.42253977152177,202.37804487904958,90.149170381246677,40.156890167033851,13.787855692755263,6.1417914812898236,8.6365417826838337E-3]
[21215.72333977852,9450.5303639143804,3244.8366478493676,1445.4104050718986,643.85713853263144,221.06814735683946,98.474664550933966,43.865476208863484,15.061197551555141,6.7090007961694509,1.7273083565367667E-2]
[26339.472235723752,11732.901025649673,4028.4879014820135,1794.4873537370956,799.35324158171397,274.45768575756449,122.25700021258915,54.459302386539427,18.698584459863085,8.3292724631654504,4.3182708913419167E-2]
[33376.737265235737,14867.646222652704,5104.8016854940379,2273.9306389836411,1012.9209457052842,347.78609024408007,154.92109099274566,69.009500689169982,23.694390501196814,10.554651062316442,8.6365417826838334E-2]
[44953.057332172939,20024.310576861026,6875.3407804304088,3062.6161440317255,1364.2403984368864,468.41151457780103,208.65360894976891,92.944616374352378,31.912504993728341,14.215404895779885,0.17273083565367667]
[72929.722568068275,32486.498175111301,11154.228998766039,4968.644158422233,2213.2793558169255,759.92877533156252,338.50978591042355,150.78896717277848,51.773344768232278,23.062403243927999,0.43182708913419171]
[112400.08741278434,50068.546897455824,17191.019934476695,7657.7288115751544,3411.1303910493239,1171.2105540376283,521.71499063227986,232.39760819444862,79.79364616628169,35.544028542642103,0.86365417826838342]
[182249.8033162014,81183.058077866386,27874.177627257985,12416.534558670131,5530.9373610322218,1899.0456148963724,845.92865200060533,376.81837585276219,129.38047162081978,57.632448159690448,1.7273083565367668]
[370168.30509412562,164891.23425226923,56615.353764046762,25219.273047725546,11233.909015324947,3857.1591506355849,1718.1690714822612,765.35731166596179,262.78519384223659,117.05749617015459,4.3182708913419168]
[]
[]
[]
[]
[]
["DIMENSIONLESS ALTERNATIVE STATE DIAGRAM FIRST GSD RESULTS",null,null,null,null,null,null,null,null,null,null,null,"GAMMAS"]
["q*W=10","q*W=32","q*W=100","q*W=316","q*W=1000","q*W=3162","q*W=10000","q*W=31623","q*W=100000","q*W=316228","q*T",null,"S",{"$f":"N2","v":"G1=1.58,G2=4.13"},{"$f":"O2","v":"G1=1.58,G2=4.13"},"G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.12","G1=1.58,G2=4.12","G1=1.58,G2=4.11","G1=1.58,G2=4.09","G1=1.55,G2=4.02","G1=1.51,G2=3.93","G1=1.45,G2=3.76","G1=1.36,G2=3.41","G1=1.3,G2=3.07","G1=1.25,G2=2.74","G1=1.2,G2=2.35","G1=1.16,G2=2.1","G1=1.13,G2=1.88","G1=1.1,G2=1.63","G1=1.08,G2=1.49","G1=1.07,G2=1.36","G1=1.05,G2=1.23"]
[9.5477690991845471E-3,3.5590204137137351E-3,1.3266582144631999E-3,4.9452428292372556E-4,1.8433856115697284E-4,6.8713926298062347E-5,2.5613760016684085E-5,9.54776909918455E-6,3.5590204137137366E-6,1.3266582144632006E-6,4.3182708913419167E-7,null,1E-4,{"$f":"N3","v":4.3182708913419167E-7},8.6365417826838334E-7,1.7273083565367667E-6,4.3182708913419169E-6,8.6365417826838338E-6,1.7273083565367668E-5,4.3182708913419166E-5,8.6365417826838331E-5,1.7273083565367666E-4,4.318270891341917E-4,8.6365417826838339E-4,1.7273083565367668E-3,4.3182708913419169E-3,8.6365417826838337E-3,1.7273083565367667E-2,4.3182708913419167E-2,8.6365417826838334E-2,0.17273083565367667,0.43182708913419171,0.86365417826838342,1.7273083565367668,4.3182708913419168]
[1.0658214261449859E-2,3.9729492550751632E-3,1.4809540694348099E-3,5.5203950893000528E-4,2.0577790068532315E-4,7.6705641037420186E-5,2.8592746584381949E-5,1.0658214261449862E-5,3.9729492550751642E-6,1.4809540694348104E-6,8.6365417826838334E-7,null,0.1,4.3182708913419167E-7,8.6365417826838334E-7,1.7273083565367667E-6,4.3182708913419169E-6,8.6365417826838338E-6,1.7273083565367668E-5,4.3182708913419166E-5,8.6365417826838331E-5,1.7273083565367666E-4,4.318270891341917E-4,8.6365417826838339E-4,1.7273083565367668E-3,4.3182708913419169E-3,8.6365417826838337E-3,1.7273083565367667E-2,4.3182708913419167E-2,8.6365417826838334E-2,0.17273083565367667,0.43182708913419171,0.86365417826838342,1.7273083565367668,4.3182708913419168]
[1.1897808803595313E-2,4.4350197381789703E-3,1.6531951725508739E-3,6.1624399436556118E-4,2.2971072435788617E-4,8.5626825360545259E-5,3.1918201650447264E-5,1.1897808803595319E-5,4.4350197381789723E-6,1.6531951725508748E-6,1.7273083565367667E-6]
[1.3760431930691482E-2,5.1293299653666757E-3,1.9120058168324071E-3,7.1271808760301186E-4,2.6567234677038606E-4,9.9031857148262437E-5,3.6915052881698926E-5,1.3760431930691489E-5,5.1293299653666784E-6,1.9120058168324081E-6,4.3182708913419169E-6]
[1.5360827259629898E-2,5.7258923231838961E-3,2.1343800267099818E-3,7.9561015843297614E-4,2.9657114303935372E-4,1.1054967304201187E-4,4.1208426701427328E-5,1.5360827259629904E-5,5.7258923231838984E-6,2.1343800267099826E-6,8.6365417826838338E-6]
[1.7147355205755666E-2,6.3918373584984515E-3,2.3826172798813261E-3,8.8814292103994957E-4,3.3106359752106842E-4,1.2340705871444075E-4,4.6001137710648646E-5,1.7147355205755672E-5,6.3918373584984532E-6,2.3826172798813272E-6,1.7273083565367668E-5]
[1.9831576650124062E-2,7.3924060584946863E-3,2.7555886401662913E-3,1.0271714910855053E-3,3.8288779998568631E-4,1.4272501588118473E-4,5.320208729305543E-5,1.9831576650124071E-5,7.3924060584946887E-6,2.7555886401662923E-6,4.3182708913419166E-5]
[2.2131644396478262E-2,8.249777867255571E-3,3.0751820171975048E-3,1.146302917613085E-3,4.2729515572732303E-4,1.5927827392101638E-4,5.9372469365058362E-5,2.2131644396478274E-5,8.2497778672555749E-6,3.0751820171975066E-6,8.6365417826838331E-5]
[2.4667485742301258E-2,9.1950364948960514E-3,3.4275360296441219E-3,1.2776461780254632E-3,4.762545869992101E-4,1.7752836077694408E-4,6.6175360280994202E-5,2.466748574230127E-5,9.1950364948960546E-6,3.4275360296441232E-6,1.7273083565367666E-4]
[2.8345824303190902E-2,1.0566171666972502E-2,3.938639515357634E-3,1.4681647924031397E-3,5.4727218605494317E-4,2.0400083640414359E-4,7.604322367190812E-5,2.8345824303190911E-5,1.0566171666972506E-5,3.9386395153576361E-6,4.318270891341917E-4]
[3.14274800122262E-2,1.1714887713889767E-2,4.3668341876490144E-3,1.6277783695537061E-3,6.0676964284128872E-4,2.2617907103329268E-4,8.4310368485036874E-5,3.1427480012226211E-5,1.1714887713889773E-5,4.3668341876490168E-6,8.6365417826838339E-4]
[3.5034216692527015E-2,1.3059332613921656E-2,4.8679886243158466E-3,1.8145883826564313E-3,6.7640482601465579E-4,2.5213623818429507E-4,9.3986145811961034E-5,3.5034216692527031E-5,1.3059332613921662E-5,4.8679886243158485E-6,1.7273083565367668E-3]
[4.1448948909806257E-2,1.545048416698486E-2,5.7593127756678172E-3,2.1468378135908964E-3,8.0025391524760829E-4,2.9830214691344291E-4,1.1119492095910145E-4,4.1448948909806275E-5,1.5450484166984865E-5,5.7593127756678198E-6,4.3182708913419169E-3]
[4.8715385436862477E-2,1.8159116483717045E-2,6.7689808571171186E-3,2.5232010535921811E-3,9.4054684024622568E-4,3.5059764953638899E-4,1.3068855967690219E-4,4.8715385436862498E-5,1.8159116483717054E-5,6.7689808571171212E-6,8.6365417826838337E-3]
[5.9141562947766582E-2,2.2045571865370546E-2,8.2176935246106968E-3,3.0632222777811583E-3,1.1418448126585873E-3,4.25633355324034E-4,1.5865882224624467E-4,5.9141562947766604E-5,2.2045571865370555E-5,8.2176935246107014E-6,1.7273083565367667E-2]
[8.0561738224444887E-2,3.0030142950309688E-2,1.1194017228173437E-2,4.1726748324836553E-3,1.5554036502482271E-3,5.7979128792202267E-4,2.1612263639514436E-4,8.0561738224444929E-5,3.00301429503097E-5,1.1194017228173442E-5,4.3182708913419167E-2]
[0.10609131134980658,3.954653059675161E-2,1.4741339911269396E-2,5.4949726082275793E-3,2.0483025387731738E-3,7.6352396808360319E-4,2.8461071487383843E-4,1.0609131134980661E-4,3.9546530596751625E-5,1.4741339911269402E-5,8.6365417826838334E-2]
[0.14489089437784602,5.400943880136741E-2,2.0132524491371127E-2,7.5045871868121734E-3,2.7974052071117021E-3,1.0427590083205898E-3,3.886981931217665E-4,1.4489089437784607E-4,5.4009438801367431E-5,2.0132524491371134E-5,0.17273083565367667]
[0.23130055957256634,8.6219451336803005E-2,3.2139108537206647E-2,1.1980153915981178E-2,4.4657146505617884E-3,1.6646369888152549E-3,6.2050903861117165E-4,2.3130055957256646E-4,8.6219451336803037E-5,3.2139108537206666E-5,0.43182708913419171]
[0.34332693344076315,0.12797833211087745,4.7705122711288662E-2,1.7782531584545323E-2,6.6286053065853241E-3,2.4708747515273743E-3,9.2104172074781792E-4,3.433269334407633E-4,1.2797833211087748E-4,4.7705122711288686E-5,0.86365417826838342]
[0.52713531045260587,0.19649462729993999,7.3245213879888096E-2,2.7302839930179554E-2,1.0177389467050131E-2,3.7937173066575486E-3,1.4141436808946788E-3,5.2713531045260609E-4,1.9649462729994007E-4,7.3245213879888132E-5,1.7273083565367668]
[0.97513080877094183,0.36348914792601922,0.13549398652116576,5.0506653329673461E-2,1.8826828378581448E-2,7.0178767237447318E-3,2.615979320537525E-3,9.751308087709422E-4,3.634891479260193E-4,1.3549398652116582E-4,4.3182708913419168]
[]
["DIMENSIONLESS ALTERNATIVE STATE DIAGRAM SECOND GSD RESULTS"]
["q*W=10","q*W=32","q*W=100","q*W=316","q*W=1000","q*W=3162","q*W=10000","q*W=31623","q*W=100000","q*W=316228","q*T"]
[2.1879591179403673E-2,8.1558226683403276E-3,3.0401593362507648E-3,1.1332478850565187E-3,4.2242876998968673E-4,1.5746428302939203E-4,5.8696287259425626E-5,2.1879591179403681E-5,8.1558226683403315E-6,3.0401593362507662E-6,4.3182708913419167E-7]
[2.4424278417345676E-2,9.1043786851721462E-3,3.3937424814216885E-3,1.2650493162113528E-3,4.7155898869981485E-4,1.7577803250354938E-4,6.5522909012954617E-5,2.4424278417345685E-5,9.1043786851721494E-6,3.3937424814216903E-6,8.6365417826838334E-7]
[2.7264923339590248E-2,1.0163255702552486E-2,3.7884488134789659E-3,1.4121798006858778E-3,5.2640325569922822E-4,1.9622174702977832E-4,7.3143495201742853E-5,2.7264923339590261E-5,1.0163255702552491E-5,3.7884488134789674E-6,1.7273083565367667E-6]
[3.1533295575953593E-2,1.1754331456975952E-2,4.3815372125523919E-3,1.6332590598836523E-3,6.0881262152697856E-4,2.2694061048524419E-4,8.459423945292351E-5,3.153329557595361E-5,1.1754331456975956E-5,4.3815372125523936E-6,4.3182708913419169E-6]
[3.5200748690795987E-2,1.3121408977019548E-2,4.8911281704422148E-3,1.8232138653395903E-3,6.7962005552309873E-4,2.5333474511679934E-4,9.4432900503496742E-5,3.5200748690796E-5,1.3121408977019553E-5,4.8911281704422172E-6,8.6365417826838338E-6]
[3.92883988711328E-2,1.4645118891326322E-2,5.4591053212573694E-3,2.0349326714056847E-3,7.5854022471955366E-4,2.8275297782708915E-4,1.0539882245486072E-4,3.9288398871132813E-5,1.4645118891326327E-5,5.4591053212573719E-6,1.7273083565367668E-5]
[4.5300924748622108E-2,1.6886344261742344E-2,6.2945430829146991E-3,2.3463499268124672E-3,8.7462392528475739E-4,3.2602426515286647E-4,1.2152860034541183E-4,4.5300924748622123E-5,1.6886344261742351E-5,6.2945430829147014E-6,4.3182708913419166E-5]
[5.0065303788547226E-2,1.8662311200784844E-2,6.9565514038608762E-3,2.5931197328079884E-3,9.6660968320398135E-4,3.6031281851067748E-4,1.3430997996293783E-4,5.0065303788547252E-5,1.8662311200784853E-5,6.956551403860879E-6,8.6365417826838331E-5]
[5.4691557245412609E-2,2.0386790534224514E-2,7.5993672372751354E-3,2.8327353592033891E-3,1.055928653628064E-3,3.9360730183645815E-4,1.4672081065956888E-4,5.469155724541263E-5,2.0386790534224519E-5,7.5993672372751401E-6,1.7273083565367666E-4]
[6.0089781832069186E-2,2.2399029341231589E-2,8.3494481113524956E-3,3.1123350347973E-3,1.1601520531226597E-3,4.3245755078305119E-4,1.6120260506016811E-4,6.0089781832069212E-5,2.2399029341231596E-5,8.3494481113524993E-6,4.318270891341917E-4]
[6.3088362639913256E-2,2.3516778440149239E-2,8.7660995635538072E-3,3.2676457684758706E-3,1.2180455846784344E-3,4.5403790725046721E-4,1.6924688518517788E-4,6.3088362639913286E-5,2.3516778440149244E-5,8.7660995635538113E-6,8.6365417826838339E-4]
[6.4878085270508576E-2,2.41839143240405E-2,9.0147807166927885E-3,3.360343998956026E-3,1.2525997188606477E-3,4.6691828460932101E-4,1.7404816656099291E-4,6.4878085270508602E-5,2.4183914324040506E-5,9.0147807166927938E-6,1.7273083565367668E-3]
[6.6605691392733188E-2,2.482789569727871E-2,9.254830808981044E-3,3.4498249206134975E-3,1.2859545710264863E-3,4.7935161835686234E-4,1.7868280824098439E-4,6.6605691392733203E-5,2.4827895697278718E-5,9.2548308089810478E-6,4.3182708913419169E-3]
[6.9202318110001437E-2,2.579581264180782E-2,9.6156309214023589E-3,3.5843165439485595E-3,1.33608758408436E-3,4.9803916882236205E-4,1.8564876781731093E-4,6.9202318110001468E-5,2.5795812641807832E-5,9.6156309214023624E-6,8.6365417826838337E-3]
[7.5088948702053293E-2,2.7990109364682457E-2,1.0433575589871872E-2,3.8892130849237636E-3,1.449740627232852E-3,5.4040440581586222E-4,2.0144080695497346E-4,7.5088948702053328E-5,2.7990109364682466E-5,1.0433575589871877E-5,1.7273083565367667E-2]
[9.1180919235834296E-2,3.3988542195603967E-2,1.2669547645099272E-2,4.7226926241102987E-3,1.7604279368611236E-3,6.5621601225105102E-4,2.4461066864371297E-4,9.1180919235834334E-5,3.398854219560398E-5,1.2669547645099278E-5,4.3182708913419167E-2]
[0.11249578560723035,4.1933858399140773E-2,1.5631238723721307E-2,5.8266907307287256E-3,2.1719535778081671E-3,8.0961605174532892E-4,3.0179197103520644E-4,1.1249578560723039E-4,4.1933858399140783E-5,1.5631238723721312E-5,8.6365417826838334E-2]
[0.14625986148904427,5.4519734122069431E-2,2.0322741854666621E-2,7.5754924917036887E-3,2.8238358240367657E-3,1.0526112684879812E-3,3.9237071543485422E-4,1.4625986148904431E-4,5.4519734122069454E-5,2.0322741854666628E-5,0.17273083565367667]
[0.22350372772697391,8.3313109194204829E-2,3.1055742265223084E-2,1.1576318984756483E-2,4.3151813951940897E-3,1.6085243070745351E-3,5.9959251060249781E-4,2.2350372772697401E-4,8.331310919420486E-5,3.1055742265223095E-5,0.43182708913419171]
[0.32541212962052857,0.12130042108877936,4.5215868792209193E-2,1.6854638856842324E-2,6.2827245960941636E-3,2.3419444750868825E-3,8.7298175186601335E-4,3.2541212962052869E-4,1.213004210887794E-4,4.5215868792209208E-5,0.86365417826838342]
[0.49476989198030424,0.18443011423466835,6.8748053565811679E-2,2.5626481275579475E-2,9.552511067661848E-3,3.5607880269055265E-3,1.3273171088465667E-3,4.9476989198030455E-4,1.8443011423466843E-4,6.8748053565811712E-5,1.7273083565367668]
[0.9134095994266116,0.34048198868980223,0.12691785229204494,4.7309818919968584E-2,1.7635178391531187E-2,6.5736780228905379E-3,2.4504000917499103E-3,9.1340959942661198E-4,3.404819886898024E-4,1.2691785229204501E-4,4.3182708913419168]
[]
[]
[]
[]
[]
["DIMENSIONED STANDARD STATE DIAGRAM FIRST GSD RESULTS",null,null,null,null,null,null,null,null,null,null,null,"GAMMAS"]
["S=0.0001","S=0.0002","S=0.0005","S=0.001","S=0.002","S=0.005","S=0.01","S=0.02","S=0.05","S=0.1","qT (kg/m-s)",null,"qW (m2/s)","G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.13","G1=1.58,G2=4.12","G1=1.58,G2=4.12","G1=1.58,G2=4.11","G1=1.58,G2=4.08","G1=1.58,G2=4.03","G1=1.58,G2=3.95","G1=1.55,G2=3.73","G1=1.51,G2=3.46","G1=1.45,G2=3.13","G1=1.36,G2=2.69","G1=1.3,G2=2.39","G1=1.25,G2=2.14","G1=1.2,G2=1.84","G1=1.16,G2=1.66","G1=1.13,G2=1.51","G1=1.1,G2=1.35","G1=1.08,G2=1.25","G1=1.07,G2=1.17","G1=1.05,G2=1.09"]
[23.318618147196801,10.38726350807084,3.5664636802347838,1.5886789605076228,0.70767602472638391,0.24298034199272264,0.10823543760730894,4.8213406310855099E-2,1.6554057993663301E-2,7.3739945232877387E-3,1.325E-5,null,5.6905782624173456E-3,1.325E-5,2.65E-5,5.3000000000000001E-5,1.325E-4,2.6499999999999999E-4,5.2999999999999998E-4,1.3249999999999998E-3,2.6499999999999996E-3,5.2999999999999992E-3,1.3250000000000001E-2,2.6500000000000003E-2,5.3000000000000005E-2,0.13250000000000001,0.26500000000000001,0.53,1.325,2.65,5.3,13.25,26.5,53,132.5]
[26.51240383150839,11.80993329415492,4.0549369068063319,1.8062690462068567,0.80460138894113087,0.27625963551375748,0.12305967757656196,5.481685450386125E-2,1.8821349867636606E-2,8.3839582353741494E-3,2.65E-5,null,5160.9250899862582,1.325E-5,2.65E-5,5.3000000000000001E-5,1.325E-4,2.6499999999999999E-4,5.2999999999999998E-4,1.3249999999999998E-3,2.6499999999999996E-3,5.2999999999999992E-3,1.3250000000000001E-2,2.6500000000000003E-2,5.3000000000000005E-2,0.13250000000000001,0.26500000000000001,0.53,1.325,2.65,5.3,13.25,26.5,53,132.5]
[30.143619681403784,13.427456067136266,4.6103128455517259,2.0536609021639864,0.91480193261641407,0.3140969577550432,0.13991428851787416,6.2324730145045831E-2,2.1399176623374441E-2,9.5322495115115046E-3,5.3000000000000001E-5]
[35.718070973678955,15.910591822448119,5.4628967313394527,2.433443847641684,1.0839760022652356,0.37218282171442291,0.1657885993896169,7.3850425339245962E-2,2.5356520467364946E-2,1.1295045790437358E-2,1.325E-4]
[40.610121738731451,18.089752700279487,6.2111109379142073,2.7667353864076039,1.2324405045920253,0.42315806220401042,0.18849548759415144,8.3965194136433871E-2,2.8829423173752769E-2,1.2842048075110874E-2,2.6499999999999999E-4]
[46.172201988452571,20.56737778261461,7.0618027358570563,3.1456755025674963,1.401239136461425,0.48111501971912246,0.21431237717291515,9.5465311052479504E-2,3.2777984723930273E-2,1.4600932286886555E-2,5.2999999999999998E-4]
[54.709866945740188,24.370475165794222,8.3675950341815568,3.7273398449349089,1.6603411449629606,0.57007761338766738,0.25394070750378844,0.11311772539938797,3.883893567485084E-2,1.7300779003329856E-2,1.3249999999999998E-3]
[62.176041883526743,27.696278006537007,9.5095084004800636,4.2360044220662392,1.8869254548278103,0.64787526538871254,0.28859562172481812,0.12855473472777734,4.4139228004815172E-2,1.9661790824597007E-2,2.6499999999999996E-3]
[70.531276218422946,31.418111785897597,10.787398865822245,4.8052399108147945,2.1404910384508491,0.73493692930495413,0.3273771841158904,0.14582995683862029,5.0070670119327677E-2,2.2303947912868414E-2,5.2999999999999992E-3]
[82.844163053162774,36.902879334735985,12.670592090126558,5.6441071255864372,2.5141639016158557,0.86323739012717593,0.38452854215755655,0.17128799264827027,5.8811678760793816E-2,2.619762460983632E-2,1.3250000000000001E-2]
[93.489858563543592,41.644997576691303,14.298796906936248,6.3693899176692765,2.8372406564937793,0.97416569297661726,0.43394148356458184,0.19329895572780154,6.6369136057332218E-2,2.956408911877953E-2,2.6500000000000003E-2]
[106.31572347424171,47.358270880682355,16.260447510880869,7.2432059219160188,3.2264814355307472,1.1078113928496403,0.49347387491550415,0.21981762129898438,7.5474311596051322E-2,3.3619983726723347E-2,5.3000000000000005E-2]
[129.64034306392369,57.748207727461718,19.827829081126001,8.832293755940448,3.9343395927031337,1.3508542699607946,0.60173716875123795,0.26804343614893744,9.2032630057737139E-2,4.0995876072761048E-2,0.13250000000000001]
[156.63469252517103,69.772823393490526,23.956477113242666,10.671397375673134,4.7535671213766877,1.6321357859820789,0.72703383978120473,0.32385675795286201,0.11119611666152723,4.9532238897969129E-2,0.26500000000000001]
[196.44778114678596,87.507538202592755,30.045685902144577,13.383831527933934,5.9618191760212991,2.0469887514537692,0.91182982735892837,0.40617401217809807,0.13945972018163111,6.2122242971012806E-2,0.53]
[281.71723988522035,125.49076394588862,43.087214594120809,19.193172125069974,8.5495862216358649,2.9354977580772945,1.3076155948874508,0.58247652865277355,0.19999313413154865,8.9086813417332808E-2,1.325]
[388.33128154021892,172.98192046898811,59.393288348808539,26.456702228046538,11.785121050593659,4.0464176307315869,1.8024741401396198,0.80291095046574879,0.27567922399137357,0.1228011336359191,2.65]
[558.50219190214841,248.7844434220969,85.420060922005334,38.050311389442122,16.949486820847365,5.8196010044610107,2.5923375374812729,1.1547550945645748,0.39648480094210309,0.17661390046072367,5.3]
[963.59472266921875,429.23265161640131,147.37689682863154,65.64894423406443,29.243280132697308,10.040671097172005,4.472610504869647,1.992321482764692,0.68406295865227851,0.30471540649530149,13.25]
[1527.3449825206392,680.35484354285813,233.59962296923311,104.05680233067818,46.352035905091924,15.914957046386846,7.0893074159423017,3.1579274446828984,1.0842734015101474,0.48298889175952786,26.5]
[2518.4010536564756,1121.820135232917,385.1765929453482,171.57666645633699,76.428716104371574,26.241775796043235,11.689382209210551,5.2070278130190832,1.7878313727841424,0.79638833913223783,53]
[5160.9250899862582,2298.9307735435359,789.3371628481807,351.60973328098822,156.6243303328495,53.776914886117787,23.954892268792236,10.670691407728462,3.6637785610317062,1.6320278117866021,132.5]
[]
["DIMENSIONED STANDARD STATE DIAGRAM SECOND GSD RESULTS"]
["S=0.0001","S=0.0002","S=0.0005","S=0.001","S=0.002","S=0.005","S=0.01","S=0.02","S=0.05","S=0.1","qT (kg/m-s)"]
[17.995188512682162,8.0159451893211493,2.7522722763558911,1.2259979214893286,0.54611998834878162,0.18751012737693698,8.3526266059222462E-2,3.7206721681605104E-2,1.2774916264995526E-2,5.6905782624173456E-3,2.9720932525120187E-6]
[20.459861809165776,9.1138323295571357,3.1292314829463566,1.3939141584606511,0.62091816848513193,0.21319205915778355,9.4966266110684386E-2,4.2302662372291529E-2,1.4524605909033362E-2,6.4699763929257116E-3,5.9441865050240374E-6]
[23.262103920453296,10.362089281989601,3.5578201175748969,1.5848286910606937,0.70596092466900173,0.24239146292386404,0.10797312180351604,4.8096557904181575E-2,1.6513938129738542E-2,7.356123155616472E-3,1.1888373010048075E-5]
[27.555477785067687,12.274569918230698,4.2144697465177341,1.8773328474069448,0.83625671363880016,0.28712848135872482,0.12790119799203511,5.6973506669858912E-2,1.9561835715035586E-2,8.7138071814985563E-3,2.9720932525120183E-5]
[31.245630146615355,13.91834592255338,4.7788597240419586,2.1287400011607382,0.94824586914408293,0.32557992291303034,0.14502936798772462,6.4603239016483696E-2,2.2181501932514995E-2,9.8807358190525375E-3,5.9441865050240365E-5]
[35.156502828444182,15.660441652079065,5.3770077484968999,2.3951846552832801,1.0669334695506423,0.36633127343141419,0.16318203095738254,7.2689331101734631E-2,2.4957859123672592E-2,1.1117462350403543E-2,1.1888373010048073E-4]
[40.215887098539305,17.914141132482637,6.1508147609769495,2.7398764930365211,1.2204762277545422,0.41905013148982351,0.18666561249041219,8.315007744429477E-2,2.8549553112171253E-2,1.2717380135556454E-2,2.9720932525120183E-4]
[43.592342376049153,19.41818097177849,6.6672263698965608,2.969911713246157,1.3229452691604899,0.45423284484246274,0.20233772960369487,9.0131211967679162E-2,3.0946523469680531E-2,1.3785109045019157E-2,5.9441865050240367E-4]
[46.116496402419756,20.542563765019661,7.0532828506684,3.1418803251708578,1.3995485771225347,0.48053456669829087,0.21405381474681537,9.5350134585493726E-2,3.2738438919974945E-2,1.4583316633860741E-2,1.1888373010048073E-3]
[47.717416951496425,21.255692797528127,7.2981354811794334,3.2509497724986427,1.4481334925288341,0.49721618222380554,0.22148462969091087,9.8660186339710104E-2,3.3874944155635675E-2,1.5089572162665701E-2,2.972093252512019E-3]
[48.4112793729443,21.564773368444961,7.4042581986386189,3.2982220689736219,1.4691909066953885,0.50444623879898776,0.22470525375836684,0.10009481126636433,3.4367522175986875E-2,1.5308990726123198E-2,5.944186505024038E-3]
[50.02700325842811,22.284496537668087,7.6513749239304456,3.4083000558703853,1.5182250754062863,0.52128210530627739,0.23220477970342995,0.10343547029192281,3.5514536408700371E-2,1.581992748092979E-2,1.1888373010048076E-2]
[56.199927246346931,25.034221571675403,8.5954921552685768,3.8288564714570588,1.705561661182218,0.5856040635034403,0.2608569547564944,0.11619856330527667,3.9896740407300853E-2,1.777197744342111E-2,2.9720932525120185E-2]
[66.176473507793304,29.478267709570588,10.121354008274986,4.5085506559083859,2.0083310000097829,0.68955982139657546,0.30716398048164523,0.13682599823499095,4.6979163745851107E-2,2.0926838380241931E-2,5.9441865050240371E-2]
[83.001012884159948,36.972747991423937,12.694581471571516,5.6547931801755826,2.5189239977835793,0.8648717676591815,0.38525657458166712,0.17161229422497262,5.8923027605834004E-2,2.6247224881492677E-2,0.11888373010048074]
[122.98151079198281,54.78203515976989,18.809394656721341,8.3786327943343952,3.7322566081205606,1.2814691403405443,0.57082960723289677,0.25427568268017053,8.7305476205653626E-2,3.889016841912437E-2,0.29720932525120186]
[177.3036696749966,78.979806017516296,27.117691720692168,12.079558396444773,5.380831545547009,1.8475068300466309,0.82297073332203263,0.36659178569180695,0.12586917508411843,5.6068343367911527E-2,0.59441865050240372]
[270.77676241310201,120.61733526801189,41.41392438016242,18.447806071723825,8.2175633909001604,2.8214978228770797,1.2568343968184743,0.55985607652013258,0.19222640895904586,8.5627130667167303E-2,1.1888373010048074]
[512.71101736386856,228.38679407294984,78.416534390751622,34.930594984864229,15.55981114794745,5.342456296342994,2.379793733066379,1.0600775931136248,0.36397731039872505,0.16213345963319631,2.9720932525120181]
[876.29719251041456,390.34602275875324,134.02518495958995,59.701432739510288,26.593964949385697,9.131029556699497,4.0674112636825672,1.811825740482188,0.62208980193131991,0.27710950355439529,5.9441865050240361]
[1558.640954709243,694.29561429574949,238.38618225176552,106.18897209523361,47.301809560141933,16.241061534113356,7.2345704509899811,3.2226347705414748,1.1064906416273754,0.49288554713005517,11.888373010048072]
[3515.4948120077697,1565.9749108233673,537.67699637839542,239.50787342353016,106.68862870877082,36.631507334750687,16.317481464038913,7.2686116597955079,2.4956755424804178,1.1116970708450005,29.720932525120187]
[]
[]
[]
[]
[]
["DIMENSIONED ALTERNATIVE STATE DIAGRAM FIRST GSD RESULTS",null,null,null,null,null,null,null,null,null,null,null,"GAMMAS"]
[3.1622776601683791E-2,0.1,0.31622776601683794,1,3.1622776601683795,10,31.622776601683793,100,316.22776601683796,1000,"qT (kg/m-s)",null,"S",{"$f":"N110","v":"G1=1.58,G2=4.13"},{"$f":"O110","v":"G1=1.58,G2=4.13"},"G1=1.58,G2=4.13","G1=1.58,G2=4.12","G1=1.58,G2=4.12","G1=1.58,G2=4.11","G1=1.58,G2=4.08","G1=1.58,G2=4.03","G1=1.58,G2=3.95","G1=1.55,G2=3.73","G1=1.51,G2=3.46","G1=1.45,G2=3.13","G1=1.36,G2=2.69","G1=1.3,G2=2.39","G1=1.25,G2=2.14","G1=1.2,G2=1.84","G1=1.16,G2=1.66","G1=1.13,G2=1.51","G1=1.1,G2=1.35","G1=1.08,G2=1.25","G1=1.07,G2=1.17","G1=1.05,G2=1.09"]
[2.8709853779009115E-2,1.0701867065779452E-2,3.9892212470044762E-3,1.4870196069280822E-3,5.5430049487703104E-4,2.0662070438710845E-4,7.701980401604351E-5,2.8709853779009123E-5,1.0701867065779455E-5,3.9892212470044778E-6,1.325E-5,null,1E-4,{"$f":"N111","v":1.325E-5},2.65E-5,5.3000000000000001E-5,1.325E-4,2.6499999999999999E-4,5.2999999999999998E-4,1.3249999999999998E-3,2.6499999999999996E-3,5.2999999999999992E-3,1.3250000000000001E-2,2.6500000000000003E-2,5.3000000000000005E-2,0.13250000000000001,0.26500000000000001,0.53,1.325,2.65,5.3,13.25,26.5,53,132.5]
[3.2048928897715954E-2,1.1946538610194599E-2,4.4531842302861363E-3,1.6599661572220127E-3,6.1876794235960961E-4,2.3065154962718782E-4,8.5977526797121516E-5,3.2048928897715964E-5,1.1946538610194604E-5,4.4531842302861385E-6,2.65E-5,null,0.1,{"$f":"N112","v":1.325E-5},2.65E-5,5.3000000000000001E-5,1.325E-4,2.6499999999999999E-4,5.2999999999999998E-4,1.3249999999999998E-3,2.6499999999999996E-3,5.2999999999999992E-3,1.3250000000000001E-2,2.6500000000000003E-2,5.3000000000000005E-2,0.13250000000000001,0.26500000000000001,0.53,1.325,2.65,5.3,13.25,26.5,53,132.5]
[3.5776352307368094E-2,1.3335970619672021E-2,4.9711080336193973E-3,1.8530271089126815E-3,6.9073322147562605E-4,2.5747728187854529E-4,9.5977069905422521E-5,3.5776352307368098E-5,1.3335970619672025E-5,4.9711080336193992E-6,5.3000000000000001E-5]
[4.1377203885240764E-2,1.5423740536681441E-2,5.7493438368300728E-3,2.1431217982099187E-3,7.9886873568773544E-4,2.9778580825055384E-4,1.1100245088336736E-4,4.1377203885240776E-5,1.5423740536681446E-5,5.7493438368300749E-6,1.325E-4]
[4.6189544381237395E-2,1.7217585557970875E-2,6.4180163804877441E-3,2.3923757556784538E-3,8.9178048435007145E-4,3.3241953333627421E-4,1.239124964974319E-4,4.6189544381237409E-5,1.721758555797088E-5,6.4180163804877469E-6,2.6499999999999999E-4]
[5.1561580044496666E-2,1.9220062198338189E-2,7.1644583154588E-3,2.670618982616238E-3,9.9549825489541645E-4,3.7108130435326361E-4,1.3832403398335026E-4,5.1561580044496683E-5,1.9220062198338194E-5,7.1644583154588033E-6,5.2999999999999998E-4]
[5.9632751736948757E-2,2.2228667089975004E-2,8.2859439855562204E-3,3.0886632767440714E-3,1.1513281834558567E-3,4.2916837066716591E-4,1.5997653234567225E-4,5.9632751736948787E-5,2.222866708997501E-5,8.2859439855562232E-6,1.3249999999999998E-3]
[6.654347702253148E-2,2.4804704707710987E-2,9.246186150272992E-3,3.446602543062058E-3,1.284753399593963E-3,4.7890387044797285E-4,1.7851590601163832E-4,6.6543477022531505E-5,2.4804704707710994E-5,9.2461861502729958E-6,2.6499999999999996E-3]
[7.4138107085952629E-2,2.7635674240963356E-2,1.0301456575728436E-2,3.839964484178237E-3,1.4313827497455193E-3,5.3356133493185297E-4,1.9888998814948319E-4,7.4138107085952655E-5,2.7635674240963366E-5,1.0301456575728439E-5,5.2999999999999992E-3]
[8.510180746266259E-2,3.1722496308527214E-2,1.1824857803237993E-2,4.4078265690967065E-3,1.6430586639202232E-3,6.1246551577380797E-4,2.2830226105078979E-4,8.5101807462662621E-5,3.1722496308527227E-5,1.1824857803237998E-5,1.3250000000000001E-2]
[9.4393263708465638E-2,3.518597370397087E-2,1.3115901462208842E-2,4.8890751926799229E-3,1.8224485986381236E-3,6.7933479518802336E-4,2.5322841165343121E-4,9.4393263708465684E-5,3.5185973703970876E-5,1.3115901462208847E-5,2.6500000000000003E-2]
[0.10538962427053299,3.9284970161718974E-2,1.4643840807758346E-2,5.4586289036291672E-3,2.0347550822697714E-3,7.5847402670477097E-4,2.8272830189666906E-4,1.0538962427053302E-4,3.9284970161718992E-5,1.4643840807758353E-5,5.3000000000000005E-2]
[0.12492070680634713,4.6565364222864343E-2,1.7357675926132712E-2,6.4702363781514111E-3,2.4118412492150484E-3,8.9903642949705552E-4,3.3512425489275898E-4,1.2492070680634719E-4,4.6565364222864358E-5,1.7357675926132719E-5,0.13250000000000001]
[0.146908465322418,5.4761507279695046E-2,2.0412865065077213E-2,7.6090867630218056E-3,2.8363584035171617E-3,1.0572791773513081E-3,3.9411072221144828E-4,1.4690846532241806E-4,5.4761507279695063E-5,2.0412865065077223E-5,0.26500000000000001]
[0.17838350009148221,6.6494121474880874E-2,2.4786306964762476E-2,9.239328219164707E-3,3.4440461849686984E-3,1.2838004931563947E-3,4.7854866564270006E-4,1.7838350009148228E-4,6.6494121474880885E-5,2.4786306964762483E-5,0.53]
[0.24297095689572518,9.0569701314341722E-2,3.3760704987014001E-2,1.2584619190299868E-2,4.6910347466316673E-3,1.7486271663323392E-3,6.5181716443925362E-4,2.4297095689572527E-4,9.0569701314341744E-5,3.3760704987014013E-5,1.325]
[0.31991205678665197,0.11925021739309603,4.4451636150069626E-2,1.6569763977072414E-2,6.176534814803584E-3,2.3023612388968443E-3,8.5822672960084037E-4,3.1991205678665209E-4,1.1925021739309608E-4,4.4451636150069645E-5,2.65]
[0.43682455345037291,0.16283044623209877,6.0696574885085099E-2,2.2625217138626873E-2,8.4337617326707484E-3,3.1437637273335939E-3,1.1718673928162594E-3,4.3682455345037303E-4,1.6283044623209884E-4,6.0696574885085123E-5,5.3]
[0.69716900066021514,0.25987627888592602,9.6871318523399211E-2,3.6109691860645124E-2,1.3460226062224826E-2,5.0174254143568768E-3,1.8702923466705282E-3,6.9716900066021535E-4,2.598762788859261E-4,9.687131852339924E-5,13.25]
[1.0346733545207103,0.38568418988885939,0.14376739642544673,5.3590644410152377E-2,1.9976414957091498E-2,7.4463958948459714E-3,2.7757138576606799E-3,1.0346733545207108E-3,3.8568418988885948E-4,1.4376739642544677E-4,26.5]
[1.588415782154436,0.59209686948080198,0.22070965724947722,8.2271593237601415E-2,3.0667507431278815E-2,1.1431600811854669E-2,4.2612363399416632E-3,1.5884157821544366E-3,5.920968694808021E-4,2.2070965724947731E-4,53]
[2.9380026984795298,1.0951680409120643,0.4082341511993427,0.15217310584287699,5.6723951374072892E-2,2.1144384493344416E-2,7.8817674857315258E-3,2.9380026984795306E-3,1.0951680409120646E-3,4.0823415119934286E-4,132.5]
[]
["DIMENSIONED ALTERNATIVE STATE DIAGRAM SECOND GSD RESULTS"]
[3.1622776601683791E-2,0.1,0.31622776601683794,1,3.1622776601683795,10,31.622776601683793,100,316.22776601683796,1000,"qT (kg/m-s)"]
[2.2991252392815069E-2,8.5702048041633293E-3,3.1946241609812163E-3,1.1908260961239966E-3,4.4389158778989653E-4,1.6546474951462464E-4,6.1678536122419938E-5,2.2991252392815077E-5,8.5702048041633331E-6,3.1946241609812176E-6,2.9720932525120187E-6]
[2.5665230442431224E-2,9.5669551827642467E-3,3.5661722061806483E-3,1.329324112132066E-3,4.9551802126467234E-4,1.8470898643690775E-4,6.8852005792795494E-5,2.5665230442431236E-5,9.5669551827642502E-6,3.5661722061806497E-6,5.9441865050240374E-6]
[2.8650203234206934E-2,1.0679631766157653E-2,3.980932830680523E-3,1.4839300220640297E-3,5.5314882316326883E-4,2.0619140796230003E-4,7.6859779750316552E-5,2.8650203234206945E-5,1.0679631766157659E-5,3.9809328306805242E-6,1.1888373010048075E-5]
[3.3126704916147207E-2,1.2348289722015638E-2,4.6029407224415023E-3,1.7157892931954858E-3,6.3957653946991025E-4,2.384081492188798E-4,8.8868871990020369E-5,3.3126704916147217E-5,1.2348289722015643E-5,4.6029407224415038E-6,2.9720932525120183E-5]
[3.6894552461057703E-2,1.3752790206766881E-2,5.1264814411553037E-3,1.9109440027361597E-3,7.1232228644728054E-4,2.6552480818012628E-4,9.897686075600679E-5,3.6894552461057719E-5,1.3752790206766888E-5,5.1264814411553059E-6,5.9441865050240365E-5]
[4.0818966127524607E-2,1.5215652180670898E-2,5.6717769519165169E-3,2.1142080148991022E-3,7.8809085197774093E-4,2.9376825108698781E-4,1.0950486879797586E-4,4.0818966127524622E-5,1.5215652180670904E-5,5.6717769519165189E-6,1.1888373010048073E-4]
[4.5804935295744253E-2,1.7074218916784841E-2,6.3645751213489742E-3,2.3724550254813136E-3,8.8435484547137657E-4,3.296515568509193E-4,1.2288070732095305E-4,4.5804935295744266E-5,1.7074218916784846E-5,6.3645751213489766E-6,2.9720932525120183E-4]
[4.9082088434930775E-2,1.8295808462999049E-2,6.8199340734760201E-3,2.5421943425251105E-3,9.47626766701677E-4,3.5323675847595223E-4,1.3167231226793649E-4,4.9082088434930787E-5,1.8295808462999055E-5,6.8199340734760223E-6,5.9441865050240367E-4]
[5.1508254532991876E-2,1.9200184614156405E-2,7.1570487596616956E-3,2.6678570012502773E-3,9.9446870045587807E-4,3.7069752828690908E-4,1.3818097785785522E-4,5.1508254532991894E-5,1.9200184614156413E-5,7.1570487596616985E-6,1.1888373010048073E-3]
[5.3037155342910439E-2,1.9770096719960089E-2,7.3694888383342228E-3,2.7470460315705695E-3,1.0239871536698532E-3,3.8170080837029145E-4,1.422825536320235E-4,5.3037155342910451E-5,1.9770096719960097E-5,7.3694888383342264E-6,2.972093252512019E-3]
[5.3697515774167912E-2,2.0016252259630076E-2,7.4612456227236799E-3,2.7812492328992125E-3,1.036736717518585E-3,3.8645332778422016E-4,1.4405409978432706E-4,5.3697515774167934E-5,2.0016252259630081E-5,7.4612456227236833E-6,5.944186505024038E-3]
[5.523002956762843E-2,2.0587511138910022E-2,7.6741877238314885E-3,2.8606253967872262E-3,1.0663249265237497E-3,3.9748260999252199E-4,1.4816536809425176E-4,5.5230029567628448E-5,2.0587511138910028E-5,7.6741877238314914E-6,1.1888373010048076E-2]
[6.1022189829750863E-2,2.274659316092455E-2,8.4790057825221126E-3,3.1606288709443496E-3,1.1781540331578255E-3,4.3916795755628309E-4,1.637039720750339E-4,6.1022189829750883E-5,2.2746593160924558E-5,8.4790057825221167E-6,2.9720932525120185E-2]
[7.019681195911015E-2,2.6166519544490771E-2,9.7538153936541951E-3,3.6358261010496573E-3,1.3552882542429857E-3,5.0519639857327526E-4,1.8831669228474643E-4,7.019681195911018E-5,2.6166519544490779E-5,9.7538153936541991E-6,5.9441865050240371E-2]
[8.523989530403038E-2,3.1773969845560662E-2,1.1844045046578818E-2,4.414978793875448E-3,1.6457247227373748E-3,6.1345931418428851E-4,2.2867270872220641E-4,8.5239895304030404E-5,3.1773969845560668E-5,1.1844045046578823E-5,0.11888373010048074]
[0.11940033996866502,4.4507595747066468E-2,1.659062344130809E-2,6.1843103755929892E-3,2.3052596520538953E-3,8.5930714026915059E-4,3.203147899889075E-4,1.1940033996866505E-4,4.4507595747066478E-5,1.6590623441308099E-5,0.29720932525120186]
[0.16337538381155683,6.0899705475000239E-2,2.2700935969764031E-2,8.4619866366163945E-3,3.1542848248040213E-3,1.1757892305024182E-3,4.3828645520347504E-4,1.6337538381155689E-4,6.0899705475000264E-5,2.2700935969764037E-5,0.59441865050240372]
[0.23486038252931879,8.7546408706705325E-2,3.2633744333124007E-2,1.2164534044651631E-2,4.5344440715400719E-3,1.6902565246192081E-3,6.3005896068919157E-4,2.3486038252931886E-4,8.7546408706705366E-5,3.2633744333124017E-5,1.1888373010048074]
[0.40594039624350337,0.15131808718594417,5.6405235156439408E-2,2.1025580036203105E-2,7.8374820108929859E-3,2.9214948726886012E-3,1.0890145941366326E-3,4.0594039624350348E-4,1.5131808718594423E-4,5.6405235156439432E-5,2.9720932525120181]
[0.64266837855060233,0.23956066121302097,8.9298481637215182E-2,3.3286845938454233E-2,1.2407983788927287E-2,4.6251922453374944E-3,1.7240837568969403E-3,6.4266837855060242E-4,2.3956066121302107E-4,8.9298481637215216E-5,5.9441865050240361]
[1.0528191743664974,0.39244821429957161,0.14628874991718951,5.4530502554403837E-2,2.0326755888741357E-2,7.576988760524702E-3,2.8243935722628761E-3,1.052819174366498E-3,3.9244821429957173E-4,1.4628874991718958E-4,11.888373010048072]
[2.114127875595269,0.78806097930116903,0.29375711576682795,0.1095007180030257,4.081741887980557E-2,1.5215075429582774E-2,5.6715619625430889E-3,2.1141278755952698E-3,7.8806097930116928E-4,2.937571157668281E-4,29.720932525120187]

{"sheet":"qt chart","index":10,"n_rows":12,"n_cols":3,"rows_kept":12,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[null,0.01,0.1]
[1,{"$f":"B$5*SQRT(1.65*9.81*($A6/1000)^3)*2650","v":3.3714936786237641E-3},3.3714936786237638E-2]
[{"$f":"2*A6","v":2},9.5360241715297684E-3,9.5360241715297694E-2]
[{"$f":"2*A7","v":4},2.6971949428990113E-2,0.26971949428990111]
[{"$f":"2*A8","v":8},7.6288193372238147E-2,0.76288193372238156]
[{"$f":"2*A9","v":16},0.2157755954319209,2.1577559543192089]
[{"$f":"2*A10","v":32},0.61030554697790518,6.1030554697790524]
[100,3.3714936786237639,33.714936786237644]

{"sheet":"SBTMzt","index":11,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["SBTMzt WORKSHEET"]
[]
["RULES, CONVENTIONS, AND UNITS"]
["1. Cells for input data are highlighted in GREEN, cells for output data are highlighted in ORANGE"]
["2. Grain-diameters must be in millimeters (mm)"]
["3. Cumulative percentiles, not fractions, are used"]
["4. Cumulative grain-size distribution percentiles must span from 0 to 100 %"]
["5. The 0 and 100 % must be EXACTLY 0 and 100"]
["INSTRUCTIONS"]
["1. In table below, enter grain size and cumulative % in order of decreasing grain size"]
["2. Check input for errors, press Enter, and then click once on the Run SBTMzt button"]
[]
["D (mm)","Surface CDF GSD (% Finer)","Transport CDF GSD (% Finer)",null,"Statistic","Surface GSD","Bedload GSD","Units"]
[64,100,100,null,"Dmin",0.21,0.21,"mm"]
[45.25,96.22,99.999997133222223,null,"Dmax",64,64,"mm"]
[32,90.93,99.999974131539986,null,"D50",5.3241924420130351,0.40700397254341353,"mm"]
[22.63,81.05,99.999714955244144,null,"Dg",4.1197847415951223,0.49788800886018231,"mm"]
[16,70.88,99.99773195434986,null,"sg",2.4162975805732634,1.0250322734546784,"f/y-units"]
[11.31,64.38,99.985265722252663,null,"Fs",34.369999999999997,93.020713833340039,"%"]
[8,58.44,99.88567065672521]
[5.66,51.51,99.313395987017117]
[4,42.94,97.361232318625355]
[2.83,36.99,94.786839660103425]
[2,34.369999999999997,93.020713833340039]
[1.41,31.5,90.281229442823076]
[1,28.17,85.985212605814255]
[0.5,17.77,65.549369694515079]
[0.21,0,0]

{"sheet":"SBTMsa","index":12,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":true,"merged":[[28,5,28,9],[27,5,27,9],[29,5,29,9]]}
["SBTMsa WORKSHEET"]
[]
["RULES, CONVENTIONS, AND UNITS"]
["1. Cells for input data are highlighted in GREEN, cells for output data are highlighted in ORANGE"]
["2. Grain-diameters must be in millimeters (mm)"]
["3. Cumulative percentiles, not fractions, are used"]
["4. Cumulative grain-size distribution percentiles must span from 0 to 100 %"]
["5. The 0 and 100 % must be EXACTLY 0 and 100"]
["INSTRUCTIONS"]
["1. In table below, enter grain size and cumulative % in order of decreasing grain size"]
["2. Check input for errors, press Enter, and then click once on the Run SBTMsa button"]
[]
["D (mm)","Surface CDF GSD (% Finer)","Transport CDF GSD (% Finer)",null,"Statistic","Surface GSD","Bedload GSD","Units"]
[64,100,100,null,"Dmin",0.21,0.21,"mm"]
[45.25,58.382478926270387,96.22,null,"Dmax",64,64,"mm"]
[32,40.766056592702796,90.93,null,"D50",38.372546666762808,5.3241924420130351,"mm"]
[22.63,25.17484335880399,81.05,null,"Dg",29.219923870263941,4.1197847415951223,"mm"]
[16,15.414499891385283,70.88,null,"sg",1.2117654396624413,2.4162975805732634,"f/y-units"]
[11.31,11.115534847666755,64.38,null,"Fs",1.7237199997926196,34.369999999999997,"%"]
[8,8.2426389831961657,58.44]
[5.66,5.7272069885623189,51.51,null,"Parameter","Value","Units"]
[4,3.3728893173052152,42.94,null,"Maximum allowed iterations",200,"#"]
[2.83,2.1351060749802415,36.99,null,"Number of iterations",28,"#"]
[2,1.7237199997926196,34.369999999999997,null,"Maximum absolute tolerance",5.0000000000000002E-5,"%"]
[1.41,1.3857074175278581,31.5,null,"Relative difference in surface Dg at convergence",4.6250951502748431E-5,"%"]
[1,1.0926072515787757,28.17,null,"Maximum absolute error from any grain size fraction percentile at convergence",4.1541964598934555E-5,"%"]
[0.5,0.50564068701476661,17.77]
[0.21,0,0,null,"Issue","Warnings"]
[null,null,null,null,"Singular derivative","No problems"]
[null,null,null,null,"Convergence","Convergence attained, have a nice day"]